1

2# -*- coding: utf-8 -*-

3

4 u'''A pure Python implementation of geodesy tools for various ellipsoidal and spherical earth

5 models using precision trigonometric, vector-based, exact, elliptic, iterative and approximate

6 methods for geodetic (lat-/longitude), geocentric (U{ECEF<https://WikiPedia.org/wiki/ECEF>}

7 cartesian) and certain U{triaxial ellipsoidal<https://GeographicLib.SourceForge.io/1.44/triaxial.html>}

8 coordinates.

9

10 Transcoded from U{JavaScript originals<https://GitHub.com/ChrisVeness/geodesy>} by I{Chris Veness

11(C) 2005-2022} and from several U{C++ classes<https://GeographicLib.SourceForge.io/C++/doc/annotated.html>}

12 by I{Charles F.F. Karney (C) 2008-2023} and published under the same U{MIT License

13<https://OpenSource.org/licenses/MIT>}**.

14

15 There are four modules for ellipsoidal earth models, C{ellipsoidalExact}, C{-Karney},

16 C{-Vincenty} and C{-Nvector} and two for spherical ones, C{sphericalTrigonometry}

17 and C{-Nvector}. Each module provides a geodetic B{C{LatLon}} and a geocentric

18 B{C{Cartesian}} class with methods and functions to compute distance, surface area,

19 perimeter, initial and final bearing, intermediate and nearest points, circle intersections

20 and secants, path intersections, U{3-point resections<https://WikiPedia.org/wiki/

21 Position_resection_and_intersection>}, rhumb and rhumb lines, trilateration (by intersection,

22 by overlap and in 3d), conversions and unrolling, among other things. For more information

23 and further details see the U{documentation<https://mrJean1.GitHub.io/PyGeodesy>}, the

24 descriptions of U{Latitude/Longitude<https://www.Movable-Type.co.UK/scripts/latlong.html>},

25 U{Vincenty<https://www.Movable-Type.co.UK/scripts/latlong-vincenty.html>} and

26 U{Vector-based<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>} geodesy,

27 the original U{JavaScript source<https://GitHub.com/ChrisVeness/geodesy>} or

28 U{docs<https://www.Movable-Type.co.UK/scripts/geodesy/docs>} and I{Karney}'s Python

29 U{geographiclib<https://PyPI.org/project/geographiclib>} and U{C++ GeographicLib

30<https://GeographicLib.SourceForge.io/C++/doc/index.html>}.

31

32 Also included are modules for conversions to and from U{Cassini-Soldner

33<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1CassiniSoldner.html>},

34 U{ECEF<https://WikiPedia.org/wiki/ECEF>} (Earth-Centered, Earth-Fixed cartesian), U{UTM

35<https://www.Movable-Type.co.UK/scripts/latlong-utm-mgrs.html>} (Universal Transverse Mercator

36 and U{Exact<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1TransverseMercatorExact.html>}),

37 U{UPS<https://WikiPedia.org/wiki/Universal_polar_stereographic_coordinate_system>} (Universal Polar

38 Stereographic) and U{Web Mercator<https://WikiPedia.org/wiki/Web_Mercator>} (Pseudo-Mercator) coordinates,

39 U{MGRS<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1MGRS.html>} (Military Grid Reference

40 System, UTM I{and} UPS) and U{OSGR<https://www.Movable-Type.co.UK/scripts/latlong-os-gridref.html>} (British

41 Ordinance Survery Grid Reference) grid references, U{TRF<http://ITRF.ENSG.IGN.Fr>} (Terrestrial Reference

42 Frames) and modules to encode and decode U{EPSG<https://EPSG.org>}, U{Geohashes

43<https://www.Movable-Type.co.UK/scripts/geohash.html>}, U{Georefs (WGRS)

44<https://WikiPedia.org/wiki/World_Geographic_Reference_System>} and U{Garefs (GARS)

45<https://WikiPedia.org/wiki/Global_Area_Reference_System>}.

46

47 Other modules provide U{Albers equal-area<https://GeographicLib.SourceForge.io/

48 html/classGeographicLib_1_1AlbersEqualArea.html>} projections, U{equidistant

49<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1AzimuthalEquidistant.html>}

50 and other I{azimuthal} projections, Lambert I{conformal conic} projections and

51 positions, functions to clip paths or polygons of C{LatLon} points using the

52 U{Cohen-Sutherland<https://WikiPedia.org/wiki/Cohen-Sutherland_algorithm>},

53 U{Forster-Hormann-Popa<https://www.ScienceDirect.com/science/article/pii/S259014861930007X>},

54 U{Greiner-Hormann<http://www.inf.USI.CH/hormann/papers/Greiner.1998.ECO.pdf>},

55 U{Liang-Barsky<https://www.CS.Helsinki.FI/group/goa/viewing/leikkaus/intro.html>} and

56 U{Sutherland-Hodgman<https://WikiPedia.org/wiki/Sutherland-Hodgman_algorithm>} methods,

57 functions to U{simplify<https://Bost.Ocks.org/mike/simplify>} or linearize a path of C{LatLon}

58 points (or a U{NumPy array<https://docs.SciPy.org/doc/numpy/reference/generated/numpy.array.html>}),

59 including implementations of the U{Ramer-Douglas-Peucker<https://WikiPedia.org/wiki/

60 Ramer-Douglas-Peucker_algorithm>}, the U{Visvalingam-Whyatt<https://hydra.Hull.ac.UK/

61 resources/hull:8338>} and the U{Reumann-Witkam<https://psimpl.SourceForge.net/reumann-witkam.html>}

62 algorithms and modified versions of the former. Other classes provide I{boolean} operations between

63(composite) polygons or U{interpolate <https://docs.SciPy.org/doc/scipy/reference/interpolate.html>}

64 the L{height<pygeodesy.heights>} of C{LatLon} points and L{Geoid<pygeodesy.geoids>} models, compute

65 various U{Fréchet<https://WikiPedia.org/wiki/Frechet_distance>} or U{Hausdorff<https://WikiPedia.org/

66 wiki/Hausdorff_distance>} distances.

67

68 Installation

69============

70

71 To install PyGeodesy, type C{python[3] -m pip install PyGeodesy} or C{python[3] -m easy_install

72 PyGeodesy} in a terminal or command window.

73

74 If the wheel C{PyGeodesy-yy.m.d-py2.py3-none-any.whl} is missing in U{PyPI Download files<https://

75 PyPI.org/project/PyGeodesy/#files>}, download the file from U{GitHub/dist<https://GitHub.com/mrJean1/

76 PyGeodesy/tree/master/dist>}. Install that with C{python[3] -m pip install <path-to-downloaded-wheel>}

77 and verify with C{python[3] -m pygeodesy}.

78

79 Alternatively, download C{PyGeodesy-yy.m.d.zip} from U{PyPI<https://PyPI.org/project/PyGeodesy>}

80 or U{GitHub<https://GitHub.com/mrJean1/PyGeodesy>}, C{unzip} the downloaded file, C{cd} to

81 directory C{Pygeodesy-yy.m.d} and type C{python[3] setup.py install}.

82

83 To run all PyGeodesy tests, type C{python[3] test/run.py} or type C{python[3] test/unitTestSuite.py}

84 before or after installation.

85

86 Dependencies

87============

88

89 Installation of I{Karney}'s Python package U{geographiclib<https://PyPI.org/project/geographiclib>}

90 is optional, but required to use modules L{ellipsoidalKarney} and L{css}, L{azimuthal} classes

91 L{EquidistantKarney} and L{GnomonicKarney} and the L{HeightIDWkarney} interpolator.

92

93 Both U{numpy<https://PyPI.org/project/numpy>} and U{scipy<https://PyPI.org/project/scipy>} must be

94 installed for most L{Geoid...<pygeodesy.geoids>} and L{Height...<pygeodesy.heights>} interpolators,

95 except L{GeoidKarney} and the L{HeightIDW...<pygeodesy.heights>} ones.

96

97 Functions and C{LatLon} methods L{circin6}, L{circum3}, L{circum4_}, L{soddy4}, L{trilaterate3d2} do and

98 C{trilaterate5} and modules L{auxilats} and L{rhumb} may require U{numpy<https://PyPI.org/project/numpy>}.

99

100 Modules L{ellipsoidalGeodSolve} and L{geodsolve} and L{azimuthal} classes L{EquidistantGeodSolve}

101 and L{GnomonicGeodSolve} depend on I{Karney}'s C++ utility U{GeodSolve

102<https://GeographicLib.SourceForge.io/C++/doc/GeodSolve.1.html>} to be executable and set with

103 env variable C{PYGEODESY_GEODSOLVE} or with property L{Ellipsoid.geodsolve}.

104

105 To compare C{MGRS} results from modules L{mgrs} and C{testMgrs} with I{Karney}'s C++ utility

106 U{GeoConvert<https://GeographicLib.SourceForge.io/C++/doc/GeoConvert.1.html>}, the latter must

107 be executable and set with env variable C{PYGEODESY_GEOCONVERT}.

108

109 Module L{rhumb.solve} needs I{Karney}'s C++ utility U{RhumbSolve

110<https://GeographicLib.SourceForge.io/C++/doc/RhumbSolve.1.html>} to be executable and set with

111 env variable C{PYGEODESY_RHUMBSOLVE} or with property L{Ellipsoid.rhumbsolve}.

112

113 Documentation

114=============

115

116 In addition to the C{pygeodesy} package, the U{PyGeodesy<https://PyPI.org/project/PyGeodesy>}

117 U{distribution files<https://GitHub.com/mrJean1/PyGeodesy/tree/master/dist>} contain the tests,

118 the test results (on macOS only) and the complete U{documentation<https://mrJean1.GitHub.io/PyGeodesy>}

119(generated by U{Epydoc<https://PyPI.org/project/epydoc>} using command line:

120 C{epydoc --html --no-private --no-source --name=PyGeodesy --url=... -v pygeodesy}).

121

122 Tests

123=====

124

125 The tests ran with Python 3.12 (with U{geographiclib<https://PyPI.org/project/geographiclib>} 2.0,

126 Python 3.11.5 (with U{geographiclib<https://PyPI.org/project/geographiclib>} 2.0, U{numpy

127<https://PyPI.org/project/numpy>} 1.24.2 and U{scipy<https://PyPI.org/project/scipy>} 1.10.1), Python

128 3.10.8 (with U{geographiclib <https://PyPI.org/project/geographiclib>} 2.0, U{numpy

129<https://PyPI.org/project/numpy>} 1.23.3, U{scipy<https://PyPI.org/project/scipy>} 1.9.1, U{GeoConvert

130<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2, U{GeodSolve

131<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2 and U{RhumbSolve

132<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2), Python 3.9.6 and Python 2.7.18 (with

133 U{geographiclib<https://PyPI.org/project/geographiclib>} 1.50, U{numpy<https://PyPI.org/project/numpy>}

134 1.16.6, U{scipy<https://PyPI.org/project/scipy>} 1.2.2, U{GeoConvert

135<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2, U{GeodSolve

136<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2 and U{RhumbSolve

137<https://GeographicLib.SourceForge.io/html/utilities.html>} 2.2), all on macOS 14.1.2 Sonoma and

138 in 64-bit only.

139

140 All tests ran with and without C{lazy import} for Python 3 and with command line option C{-W default} and

141 env variable C{PYGEODESY_WARNINGS=on} for all Python versions. The results of those tests are included in

142 the distribution files.

143

144 Test coverage has been measured with U{coverage<https://PyPI.org/project/coverage>} 7.2.2 using only Python 3.11.5

145 and 3.10.8. The complete coverage report in HTML and a PDF summary are included in the distribution files.

146

147 PyPy 7.3.12 (Python 3.10.12), Python 3.11.5, 3.10.8 and 3.9.6 ran on Apple M1 Silicon (C{arm64}), I{natively}.

148 Python 3.8.10 and 2.7.18 ran on Intel (C{x86_64}) or Intel I{emulation} ("C{arm64_x86_64}", see function

149 L{pygeodesy.machine}).

150

151 The tests also ran with Python 3.11.5 (and U{geographiclib<https://PyPI.org/project/geographiclib>} 2.0) on

152 U{Debian 11<https://Cirrus-CI.com/github/mrJean1/PyGeodesy/master>} in 64-bit only and with Python 3.11.5,

153 3.10.10 and 2.7.18 (all with U{geographiclib<https://PyPI.org/project/geographiclib>} 1.52) on U{Windows 10

154<https://CI.AppVeyor.com/project/mrJean1/pygeodesy>} in 64- and/or 32-bit.

155

156 A single-File and single-Directory application with C{pygeodesy} has been bundled using U{PyInstaller

157<https://PyPI.org/project/pyinstaller>} 3.4 and 64-bit Python 3.7.3 on macOS 10.13.6 High Sierra.

158

159 Previously, the tests were run with Python 3.11.2-4, 3.10.1-7, 3.9.1, 3.8.7, 3.7.1, 2.7.15, U{PyPy

160<https://PyPy.org>} 7.3.12 (Python 3.10.12), 7.3.1 (Python 3.6.9) and U{PyPy<https://PyPy.org>} 7.1.1 (Python

161 2.7.13) (and U{geographiclib <https://PyPI.org/project/geographiclib>} 1.52, U{numpy<https://PyPI.org/project/numpy>}

162 1.16.3, 1.16.4, 1.16.6, 1.19.0, 1.19.4, 1.19.5 or 1.22.4 and U{scipy<https://PyPI.org/project/scipy>} 1.2.1, 1.4.1,

163 1.5.2 or 1.8.1) on U{Ubuntu 16.04<https://Travis-CI.com/mrJean1/PyGeodesy>}, with Python 3.10.0-1, 3.9.0-5, 3.8.0-6,

164 3.7.2-6, 3.7.0, 3.6.2-5, 3.5.3, 2.7.13-17, 2.7.10 and 2.6.9 (and U{numpy<https://PyPI.org/project/numpy>} 1.19.0,

165 1.16.5, 1.16.2, 1.15.2, 1.14.0, 1.13.1, 1.8.0rc1 or 1.6.2 and U{scipy<https://PyPI.org/project/scipy>} 1.5.0), U{PyPy

166<https://PyPy.org>} 7.3.0 (Python 2.7.13 and 3.6.9), U{PyPy<https://PyPy.org>} 6.0.0 (Python 2.7.13 and 3.5.3)

167 and U{Intel-Python<https://software.Intel.com/en-us/distribution-for-python>} 3.5.3 (and U{numpy

168<https://PyPI.org/project/numpy>} 1.11.3) on macOS 14.0 Sonoma, 13.0-5.2 Ventura, 12.1-6 Monterey, 11.0-5.2-6.1

169 Big Sur (aka 10.16), 10.15.3, 10.15.5-7 Catalina, 10.14 Mojave, 10.13.6 High Sierra and 10.12 Sierra, MacOS X

170 10.11 El Capitan and/or MacOS X 10.10 Yosemite, with U{Pythonista<https://OMZ-Software.com/pythonista>}3.2 (with

171 geographiclib 1.50 or 1.49 and numpy 1.8.0) on iOS 14.4.2, 11.4.1, 12.0-3 on iPad4, iPhone6, iPhone10 and/or

172 iPhone12, with U{Pythonista<https://OMZ-Software.com/pythonista>} 3.1 on iOS 10.3.3, 11.0.3, 11.1.2 and 11.3

173 on iPad4, all in 64-bit only and with 32-bit Python 2.7.14 on Windows Server 2012R2, Windows 10 Pro and with

174 32-bit Python 2.6.6 on Windows XP SP3.

175

176 Notes

177=====

178

179 All Python source code has been statically U{checked<https://GitHub.com/ActiveState/code/tree/master/recipes/

180 Python/546532_PyChecker_postprocessor>} with U{PyChecker<https://PyPI.org/project/pychecker>}, U{PyFlakes

181<https://PyPI.org/project/pyflakes>}, U{PyCodeStyle<https://PyPI.org/project/pycodestyle>} (formerly Pep8) and

182 U{McCabe<https://PyPI.org/project/mccabe>} using Python 2.7.18 and with U{Flake8<https://PyPI.org/project/flake8>}

183 using Python 3.11.5, both in 64-bit on macOS 14.1.2 Sonoma.

184

185 For a summary of all I{Karney}-based functionality in C{pygeodesy}, see module U{karney

186<https://mrJean1.GitHub.io/PyGeodesy/docs/pygeodesy.karney-module.html>}.

187

188 In Python 2, symbols L{S_DEG}, L{S_MIN}, L{S_SEC}, L{S_RAD} and L{S_SEP} may be multi-byte, non-ascii

189 characters and if so, I{not} C{unicode}.

190

191 Env variables

192=============

193

194 The following environment variables are observed by C{PyGeodesy}:

195

196 - C{PYGEODESY_EXCEPTION_CHAINING} - see module L{pygeodesy.errors}.

197 - C{PYGEODESY_FMT_FORM} - see module L{pygeodesy.dms}.

198 - C{PYGEODESY_FSUM_PARTIALS} - see module L{pygeodesy.fsums} and class L{pygeodesy.Fsum}.

199 - C{PYGEODESY_FSUM_RESIDUAL} - see module L{pygeodesy.fsums} and class L{pygeodesy.Fsum}.

200 - C{PYGEODESY_GEOCONVERT} - see module L{pygeodesy.mgrs}.

201 - C{PYGEODESY_GEODSOLVE} - see module L{pygeodesy.geodsolve}.

202 - C{PYGEODESY_LAZY_IMPORT} - see module L{pygeodesy.lazily} and variable L{pygeodesy.isLazy}.

203 - C{PYGEODESY_NOTIMPLEMENTED} - __special__ methods return C{NotImplemented} if set to "std".

204 - C{PYGEODESY_RHUMBSOLVE} - see module L{pygeodesy.rhumb.solve}.

205 - C{PYGEODESY_UPS_POLES} - see modules L{pygeodesy.ups} and L{pygeodesy.mgrs}.

206

207 and these to control standard or I{named} C{repr}esentations:

208

209 - C{PYGEODESY_BEARING_STD_REPR} - see method L{pygeodesy.Bearing}C{.__repr__}.

210 - C{PYGEODESY_BOOL_STD_REPR} - see method L{pygeodesy.Bool}C{.__repr__}.

211 - C{PYGEODESY_DEGREES_STD_REPR} - see method L{pygeodesy.Degrees}C{.__repr__}.

212 - C{PYGEODESY_FLOAT_STD_REPR} - see method L{pygeodesy.Float}C{.__repr__}.

213 - C{PYGEODESY_INT_STD_REPR} - see method L{pygeodesy.Int}C{.__repr__}.

214 - C{PYGEODESY_METER_STD_REPR} - see method L{pygeodesy.Meter}C{.__repr__}.

215 - C{PYGEODESY_RADIANS_STD_REPR} - see method L{pygeodesy.Radians}C{.__repr__}.

216 - C{PYGEODESY_STR_STD_REPR} - see method L{pygeodesy.Str}C{.__repr__}.

217

218 plus during development:

219

220 - C{PYGEODESY_FOR_DOCS} - for extended documentation by C{epydoc}.

221 - C{PYGEODESY_GEOGRAPHICLIB} - see module L{pygeodesy.karney}.

222 - C{PYGEODESY_WARNINGS} - see module L{pygeodesy.props} and function L{pygeodesy.DeprecationWarnings}.

223 - C{PYGEODESY_XPACKAGES} - see module L{pygeodesy.basics}.

224 - C{PYTHONDEVMODE} - see modules L{pygeodesy.errors} and L{pygeodesy.props}.

225

226 and:

227

228 - C{PYGEODESY_INIT__ALL__} - Set env variable C{PYGEODESY_INIT__ALL__} to anything

229 other than C{"__all__"} to avoid importing all C{pygeodesy} modules unnecessarily

230 (in Python 2 or with C{PYGEODESY_LAZY_IMPORT} turned off in Python 3). However,

231 to import a C{pygeodesy} item, the item name must be qualified with the C{module}

232 name, for example C{ from pygeodesy.ellipsoidalExact import LatLon } or C{ from

233 pygeodesy.deprecated import collins }

234

235 License

236=======

237

238**) U{Copyright (C) 2016-2023 -- mrJean1 at Gmail -- All Rights Reserved.

239<https://OpenSource.org/licenses/MIT>}

240

241 C{Permission is hereby granted, free of charge, to any person obtaining a

242 copy of this software and associated documentation files (the "Software"),

243 to deal in the Software without restriction, including without limitation

244 the rights to use, copy, modify, merge, publish, distribute, sublicense,

245 and/or sell copies of the Software, and to permit persons to whom the

246 Software is furnished to do so, subject to the following conditions:}

247

248 C{The above copyright notice and this permission notice shall be included

249 in all copies or substantial portions of the Software.}

250

251 C{THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

252 OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

253 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

254 THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

255 OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

256 ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

257 OTHER DEALINGS IN THE SOFTWARE.}

258

259@newfield example: Example, Examples

260

261@var EPS: System's M{epsilon} ≈ 2.22044604925e-16 (C{float}).

262@var EPS0: M{EPS**2} ≈ 4.9e-32 for near-zero comparison

263@var EPS02: M{EPS**4} ≈ 2.4e-63 for near-zero squared comparison

264@var EPS1: M{1 - EPS} ≈ 0.9999999999999998 (C{float}).

265@var EPS2: M{EPS * 2} ≈ 4.440892098501e-16 (C{float}).

266@var EPS_2: M{EPS / 2} ≈ 1.110223024625e-16 (C{float}).

267@var EPS4: M{EPS * 4} ≈ 8.881784197001e-16 (C{float}).

268

269@var F_D: Format degrees as unsigned "deg°" with symbol, plus compass point suffix C{N, S, E} or C{W} (C{str}).

270@var F_DM: Format degrees as unsigned "deg°min′" with symbols, plus suffix (C{str}).

271@var F_DMS: Format degrees as unsigned "deg°min′sec″" with symbols, plus suffix (C{str}).

272@var F_DEG: Format degrees as unsigned "[D]DD" I{without} symbol, plus suffix (C{str}).

273@var F_MIN: Format degrees as unsigned "[D]DDMM" I{without} symbols, plus suffix (C{str}).

274@var F_SEC: Format degrees as unsigned "[D]DDMMSS" I{without} symbols, plus suffix (C{str}).

275@var F_D60: Format degrees as unsigned "[D]DD.MMSS" C{sexagecimal} I{without} symbols, plus suffix (C{str}).

276@var F__E: Format degrees as unsigned "%E" I{without} symbols, plus suffix (C{str}).

277@var F__F: Format degrees as unsigned "%F" I{without} symbols, plus suffix (C{str}).

278@var F__G: Format degrees as unsigned "%G" I{without} symbols, plus suffix (C{str}).

279@var F_RAD: Convert degrees to radians and format as unsigned "RR" with symbol, plus suffix (C{str}).

280

281@var F_D_: Format degrees as signed "-/deg°" with symbol, I{without} suffix (C{str}).

282@var F_DM_: Format degrees as signed "-/deg°min′" with symbols, I{without} suffix (C{str}).

283@var F_DMS_: Format degrees as signed "-/deg°min′sec″" with symbols, I{without} suffix (C{str}).

284@var F_DEG_: Format degrees as signed "-/[D]DD" I{without} symbol, I{without} suffix (C{str}).

285@var F_MIN_: Format degrees as signed "-/[D]DDMM" I{without} symbols, I{without} suffix (C{str}).

286@var F_SEC_: Format degrees as signed "-/[D]DDMMSS" I{without} symbols, I{without} suffix (C{str}).

287@var F_D60_: Format degrees as signed "-/[D]DD.MMSS" C{sexagecimal} I{without} symbols, I{without} suffix (C{str}).

288@var F__E_: Format degrees as signed "-/%E" I{without} symbols, I{without} suffix (C{str}).

289@var F__F_: Format degrees as signed "-/%F" I{without} symbols, I{without} suffix (C{str}).

290@var F__G_: Format degrees as signed "-/%G" I{without} symbols, I{without} suffix (C{str}).

291@var F_RAD_: Convert degrees to radians and format as signed "-/RR" I{without} symbol, I{without} suffix (C{str}).

292

293@var F_D__: Format degrees as signed "-/+deg°" with symbol, I{without} suffix (C{str}).

294@var F_DM__: Format degrees as signed "-/+deg°min′" with symbols, I{without} suffix (C{str}).

295@var F_DMS__: Format degrees as signed "-/+deg°min′sec″" with symbols, I{without} suffix (C{str}).

296@var F_DEG__: Format degrees as signed "-/+[D]DD" I{without} symbol, I{without} suffix (C{str}).

297@var F_MIN__: Format degrees as signed "-/+[D]DDMM" I{without} symbols, without suffix (C{str}).

298@var F_SEC__: Format degrees as signed "-/+[D]DDMMSS" I{without} symbols, I{without} suffix (C{str}).

299@var F_D60__: Format degrees as signed "-/+[D]DD.MMSS" C{sexagecimal} I{without} symbols, I{without} suffix (C{str}).

300@var F__E__: Format degrees as signed "-/+%E" I{without} symbols, I{without} suffix (C{str}).

301@var F__F__: Format degrees as signed "-/+%F" I{without} symbols, I{without} suffix (C{str}).

302@var F__G__: Format degrees as signed "-/+%G" I{without} symbols, I{without} suffix (C{str}).

303@var F_RAD__: Convert degrees to radians and format as signed "-/+RR" I{without} symbol, I{without} suffix (C{str}).

304

305@var DIG: System's M{float decimal digits} = 15 (C{int}).

306@var INF: Infinity (C{float}), see functions L{pygeodesy.isinf} and L{pygeodesy.isfinite} and C{NINF}.

307@var INT0: C{int(0)}, missing Z-components, C{if B{z}=B{INT0}}, see functions L{pygeodesy.isint0}, L{pygeodesy.meeus2}

308@var MANT_DIG: System's M{float mantissa bits} = 53 (C{int}).

309@var MAX: System's M{float max} ≈ 1.798e+308 (C{float}).

310@var MIN: System's M{float min} ≈ 2.225e-308 (C{float}).

311@var NAN: Not-A-Number (C{float}), see function L{pygeodesy.isnan}.

312@var NEG0: Negative 0.0 (C{float}), see function L{pygeodesy.isneg0}.

313@var NINF: Negative infinity (C{float}), see function L{pygeodesy.isninf} and C{INF}.

314@var NN: Empty (C{str}), U{I{Nomen Nescio}<https://Wiktionary.org/wiki/N.N.>}.

315

316@var PI: Constant M{math.pi} (C{float}).

317@var PI2: Two PI, M{PI * 2}, aka I{Tau} (C{float}).

318@var PI_2: Half PI, M{PI / 2} (C{float}).

319@var PI3: Three PI, M{PI * 3} (C{float}).

320@var PI3_2: One and a half PI, M{PI * 3 / 2} (C{float}).

321@var PI_3: One third PI, M{PI / 3} (C{float}).

322@var PI4: Four PI, M{PI * 4} (C{float}).

323@var PI_4: Quarter PI, M{PI / 4} (C{float}).

324

325@var R_MA: Equatorial earth radius (C{meter}), WGS84, EPSG:3785.

326@var R_MB: Polar earth radius (C{meter}), WGS84, EPSG:3785.

327@var R_M: Mean (spherical) earth radius (C{meter}).

328@var R_KM: Mean (spherical) earth radius (C{Km}, kilometer).

329@var R_NM: Mean (spherical) earth radius (C{NM}, nautical miles).

330@var R_SM: Mean (spherical) earth radius (C{SM}, statute miles).

331@var R_FM: Former FAI-Sphere earth radius (C{meter}).

332@var R_GM: Average earth radius, distance to geoid surface (C{meter})

333@var R_QM: Earth' (triaxial) quadratic mean radius (C{meter})

334@var R_VM: Aviation/Navigation earth radius (C{meter}).

335

336@var S_DEG: Degrees symbol, default C{"°"}

337@var S_MIN: Minutes symbol, default C{"′"} aka I{PRIME}

338@var S_SEC: Seconds symbol, default C{"″"} aka I{DOUBLE_PRIME}

339@var S_RAD: Radians symbol, default C{""} aka L{pygeodesy.NN}

340@var S_DMS: If C{True} include, otherwise cancel all DMS symbols, default C{True}.

341@var S_SEP: Separator between C{deg°|min′|sec″|suffix}, default C{""} aka L{pygeodesy.NN}

342

343@var Conics: Registered, predefined conics (C{enum-like}).

344@var Datums: Registered, predefined datums (C{enum-like}).

345@var Ellipsoids: Registered, predefined ellipsoids (C{enum-like}).

346@var RefFrames: Registered, predefined reference frames (C{enum-like}).

347@var Transforms: Registered, predefined transforms (C{enum-like}).

348

349@var isLazy: Lazy import setting (C{int} 0, 1, 2 or 3+) from C{env} variable C{PYGEODESY_LAZY_IMPORT}, or C{None} if C{lazy import} is not supported or not enabled, or C{False} if initializing C{lazy import} failed.

350

351@var pygeodesy_abspath: Fully qualified C{pygeodesy} directory name (C{str}).

352

353@var version: Normalized C{PyGeodesy} version (C{str}).

354'''

355

356 from os.path import abspath, basename, dirname

357 import sys

358

359_init__all__ = True

360# <https://PyInstaller.ReadTheDocs.io/en/stable/runtime-information.html>

361_isfrozen = getattr(sys, 'frozen', False)

362 pygeodesy_abspath = dirname(abspath(__file__)) # sys._MEIPASS + '/pygeodesy'

363_pygeodesy_ = __package__ or basename(pygeodesy_abspath)

364

365 if _isfrozen: # avoid lazy import

366 _lazy_import2 = None

367 else:

368 # setting __path__ should ...

369 __path__ = [pygeodesy_abspath]

370 try: # ... make this import work, ...

371 import pygeodesy.lazily as _

372 except ImportError: # ... if it doesn't, extend

373 # sys.path to include this very directory such

374 # that all public and private sub-modules can

375 # be imported (and checked by PyChecker, etc.)

376 sys.path.insert(0, pygeodesy_abspath) # XXX __path__[0]

377

378 try: # lazily requires Python 3.7+, see lazily.__doc__

379 from pygeodesy.lazily import _init__all__, _lazy_import2 # PYCHOK expected

380 _, __getattr__ = _lazy_import2(_pygeodesy_) # PYCHOK expected

381

382 except (ImportError, NotImplementedError): # LazyImportError

383 _lazy_import2 = None

384

385 if _init__all__ and not _lazy_import2: # import and set __all__

386

387 # import all public modules and export as such

388 import pygeodesy.albers as albers # PYCHOK exported

389 import pygeodesy.auxilats as auxilats # PYCHOK exported

390 import pygeodesy.azimuthal as azimuthal # PYCHOK exported

391 import pygeodesy.basics as basics # PYCHOK exported

392 import pygeodesy.booleans as booleans # PYCHOK exported

393 import pygeodesy.cartesianBase as cartesianBase # PYCHOK INTERNAL

394 import pygeodesy.clipy as clipy # PYCHOK exported

395 import pygeodesy.constants as constants # PYCHOK exported

396 import pygeodesy.css as css # PYCHOK exported

397 import pygeodesy.datums as datums # PYCHOK exported

398 import pygeodesy.deprecated as deprecated # PYCHOK exported

399 import pygeodesy.dms as dms # PYCHOK exported

400 import pygeodesy.ecef as ecef # PYCHOK exported

401 import pygeodesy.elevations as elevations # PYCHOK exported

402 import pygeodesy.ellipsoidalBase as ellipsoidalBase # PYCHOK INTERNAL

403 import pygeodesy.ellipsoidalBaseDI as ellipsoidalBaseDI # PYCHOK INTERNAL

404 import pygeodesy.ellipsoidalExact as ellipsoidalExact # PYCHOK exported

405 import pygeodesy.ellipsoidalGeodSolve as ellipsoidalGeodSolve # PYCHOK exported

406 import pygeodesy.ellipsoidalKarney as ellipsoidalKarney # PYCHOK exported

407 import pygeodesy.ellipsoidalNvector as ellipsoidalNvector # PYCHOK exported

408 import pygeodesy.ellipsoidalVincenty as ellipsoidalVincenty # PYCHOK exported

409 import pygeodesy.ellipsoids as ellipsoids # PYCHOK exported

410 import pygeodesy.elliptic as elliptic # PYCHOK exported

411 import pygeodesy.epsg as epsg # PYCHOK exported

412 import pygeodesy.etm as etm # PYCHOK exported

413 import pygeodesy.errors as errors # PYCHOK exported

414 import pygeodesy.fmath as fmath # PYCHOK exported

415 import pygeodesy.formy as formy # PYCHOK exported

416 import pygeodesy.frechet as frechet # PYCHOK exported

417 import pygeodesy.fstats as fstats # PYCHOK exported

418 import pygeodesy.fsums as fsums # PYCHOK exported

419 import pygeodesy.gars as gars # PYCHOK exported

420 import pygeodesy.geodesicw as geodesicw # PYCHOK exported

421 import pygeodesy.geodesicx as geodesicx # PYCHOK exported

422 import pygeodesy.geodsolve as geodsolve # PYCHOK exported

423 import pygeodesy.geohash as geohash # PYCHOK exported

424 import pygeodesy.geoids as geoids # PYCHOK exported

425 import pygeodesy.hausdorff as hausdorff # PYCHOK exported

426 import pygeodesy.heights as heights # PYCHOK exported

427 import pygeodesy.interns as interns # PYCHOK exported

428 import pygeodesy.iters as iters # PYCHOK exported

429 import pygeodesy.karney as karney # PYCHOK exported

430 import pygeodesy.ktm as ktm # PYCHOK exported

431 import pygeodesy.latlonBase as latlonBase # PYCHOK INTERNAL

432 import pygeodesy.lazily as lazily # PYCHOK exported

433 import pygeodesy.lcc as lcc # PYCHOK exported

434 import pygeodesy.ltp as ltp # PYCHOK exported

435 import pygeodesy.ltpTuples as ltpTuples # PYCHOK exported

436 import pygeodesy.mgrs as mgrs # PYCHOK exported

437 import pygeodesy.named as named # PYCHOK exported

438 import pygeodesy.namedTuples as namedTuples # PYCHOK exported

439 import pygeodesy.nvectorBase as nvectorBase # PYCHOK INTERNAL

440 import pygeodesy.osgr as osgr # PYCHOK exported

441 import pygeodesy.points as points # PYCHOK exported

442 import pygeodesy.props as props # PYCHOK exported

443 import pygeodesy.resections as resections # PYCHOK exported

444 import pygeodesy.rhumb as rhumb # PYCHOK exported

445 import pygeodesy.simplify as simplify # PYCHOK exported

446 import pygeodesy.sphericalBase as sphericalBase # PYCHOK INTERNAL

447 import pygeodesy.sphericalNvector as sphericalNvector # PYCHOK exported

448 import pygeodesy.sphericalTrigonometry as sphericalTrigonometry # PYCHOK exported

449 import pygeodesy.solveBase as solveBase # PYCHOK exported

450 import pygeodesy.streprs as streprs # PYCHOK exported

451 import pygeodesy.trf as trf # PYCHOK exported

452 import pygeodesy.triaxials as triaxials # PYCHOK exported

453 import pygeodesy.units as units # PYCHOK exported

454 import pygeodesy.unitsBase as unitsBase # PYCHOK INTERNAL

455 import pygeodesy.ups as ups # PYCHOK exported

456 import pygeodesy.utily as utily # PYCHOK exported

457 import pygeodesy.utm as utm # PYCHOK exported

458 import pygeodesy.utmups as utmups # PYCHOK exported

459 import pygeodesy.utmupsBase as utmupsBase # PYCHOK INTERNAL

460 import pygeodesy.vector2d as vector2d # PYCHOK exported

461 import pygeodesy.vector3d as vector3d # PYCHOK exported

462 import pygeodesy.vector3dBase as vector3dBase # PYCHOK INTERNAL

463 import pygeodesy.webmercator as webmercator # PYCHOK exported

464 import pygeodesy.wgrs as wgrs # PYCHOK exported

465

466 # lift all public classes, constants, functions, etc. but ONLY

467 # from the following modules ... (see also David Beazley's

468 # talk <https://DaBeaz.com/modulepackage/index.html>) ... BUT

469 # NOT modules ellipsoidal*, epsg, gars, geohash, spherical*,

470 # vector and wgrs ... in order keep those as modules ONLY

471 from pygeodesy.albers import * # PYCHOK __all__

472 from pygeodesy.azimuthal import * # PYCHOK __all__

473# from pygeodesy.auxilats import * # PYCHOK __(_)__

474 from pygeodesy.basics import * # PYCHOK __all__

475 from pygeodesy.booleans import * # PYCHOK __all__

476 from pygeodesy.cartesianBase import * # PYCHOK __(_)__ INTERNAL

477 from pygeodesy.clipy import * # PYCHOK __all__

478 from pygeodesy.constants import * # PYCHOK __all__

479 from pygeodesy.css import * # PYCHOK __all__

480 from pygeodesy.datums import * # PYCHOK __all__

481 from pygeodesy.deprecated import * # PYCHOK __all__ DEPRECATED

482 from pygeodesy.dms import * # PYCHOK __all__

483 from pygeodesy.ecef import * # PYCHOK __all__

484 from pygeodesy.elevations import * # PYCHOK __all__

485# from pygeodesy.ellipsoidalBase import * # PYCHOK __(_)__ INTERNAL

486# from pygeodesy.ellipsoidalBaseDI import * # PYCHOK __(_)__ INTERNAL

487# from pygeodesy.ellipsoidalExact import * # PYCHOK __(_)__

488# from pygeodesy.ellipsoidalGeodSolve import * # PYCHOK __(_)__

489# from pygeodesy.ellipsoidalKarney import * # PYCHOK __(_)__

490# from pygeodesy.ellipsoidalNvector import * # PYCHOK __(_)__

491 from pygeodesy.ellipsoidalVincenty import VincentyError # PYCHOK lazily

492 from pygeodesy.ellipsoids import * # PYCHOK __all__

493 from pygeodesy.elliptic import * # PYCHOK __all__

494 from pygeodesy.epsg import Epsg, EPSGError # PYCHOK lazily

495 from pygeodesy.etm import * # PYCHOK __all__

496 from pygeodesy.errors import * # PYCHOK __all__

497 from pygeodesy.fmath import * # PYCHOK __all__

498 from pygeodesy.formy import * # PYCHOK __all__

499 from pygeodesy.frechet import * # PYCHOK __all__

500 from pygeodesy.fstats import * # PYCHOK __all__

501 from pygeodesy.fsums import * # PYCHOK __all__

502 from pygeodesy.gars import Garef, GARSError # PYCHOK lazily

503 from pygeodesy.geodesicw import * # PYCHOK __all__

504 from pygeodesy.geodesicx import * # PYCHOK __all__

505 from pygeodesy.geodsolve import * # PYCHOK __all__

506 from pygeodesy.geohash import Geohash, GeohashError, \

507 Neighbors8Dict, Resolutions2Tuple # PYCHOK lazily

508 from pygeodesy.geoids import * # PYCHOK __all__

509 from pygeodesy.hausdorff import * # PYCHOK __all__

510 from pygeodesy.heights import * # PYCHOK __all__

511 from pygeodesy.interns import * # PYCHOK __all__

512 from pygeodesy.iters import * # PYCHOK __all__

513 from pygeodesy.karney import * # PYCHOK __all__

514 from pygeodesy.ktm import * # PYCHOK __all__

515 from pygeodesy.latlonBase import * # PYCHOK __(_)__ INTERNAL

516 from pygeodesy.lazily import * # PYCHOK __all__

517 from pygeodesy.lcc import * # PYCHOK __all__

518 from pygeodesy.ltp import * # PYCHOK __all__

519 from pygeodesy.ltpTuples import * # PYCHOK __all__

520 from pygeodesy.mgrs import * # PYCHOK __all__

521 from pygeodesy.named import * # PYCHOK __all__

522 from pygeodesy.namedTuples import * # PYCHOK __all__

523# from pygeodesy.nvectorBase import * # PYCHOK __(_)__ INTERNAL

524 from pygeodesy.osgr import * # PYCHOK __all__

525 from pygeodesy.points import * # PYCHOK __all__

526 from pygeodesy.props import * # PYCHOK __all__

527 from pygeodesy.resections import * # PYCHOK __all__

528 from pygeodesy.rhumb import * # PYCHOK __all__

529 from pygeodesy.simplify import * # PYCHOK __all__

530# from pygeodesy.sphericalBase import * # PYCHOK __(_)__ INTERNAL

531# from pygeodesy.sphericalNvector import * # PYCHOK __(_)__

532# from pygeodesy.sphericalTrigonometry import * # PYCHOK __(_)__

533# from pygeodesy.solveBase import * # PYCHOK __(_)__ INTERNAL

534 from pygeodesy.streprs import * # PYCHOK __all__

535 from pygeodesy.trf import * # PYCHOK __all__

536 from pygeodesy.triaxials import * # PYCHOK __all__

537 from pygeodesy.units import * # PYCHOK __all__

538 from pygeodesy.unitsBase import * # PYCHOK __all__ Float, ...

539 from pygeodesy.ups import * # PYCHOK __all__

540 from pygeodesy.utily import * # PYCHOK __all__

541 from pygeodesy.utm import * # PYCHOK __all__

542 from pygeodesy.utmups import * # PYCHOK __all__

543# from pygeodesy.utmupsBase import * # PYCHOK __(_)__ INTERNAL

544 from pygeodesy.vector2d import * # PYCHOK __all__

545 from pygeodesy.vector3d import * # PYCHOK __all__

546 from pygeodesy.vector3dBase import * # PYCHOK __(_)__ INTERNAL

547 from pygeodesy.webmercator import * # PYCHOK __all__

548 from pygeodesy.wgrs import Georef, WGRSError # PYCHOK lazily

549

550 def _all(globalocals):

551 from pygeodesy.interns import NN as _NN, _attribute_, _COMMASPACE_, _DOT_, \

552 _headof, _module_, _s_, _tailof, _UNDER_ # PYCHOK expected

553 from pygeodesy.streprs import Fmt as _Fmt # PYCHOK expected

554 # collect all public module and attribute names and check

555 # that modules are imported from this package, 'pygeodesy'

556 # (but the latter only when not bundled with PyInstaller or

557 # Py2Exe, since the file-layout is different. Courtesy of

558 # GilderGeek<https://GitHub.com/mrJean1/PyGeodesy/issues/31>)

559 ns = list(lazily._ALL_INIT)

560# XXX ps = () if _isfrozen else set([_pygeodesy_] + __name__.split(_DOT_))

561 for mod, attrs in lazily._ALL_LAZY.enums():

562 mod = _headof(_headof(mod))

563 if mod not in globalocals:

564 t = _DOT_(_pygeodesy_, mod)

565 raise ImportError('missing %s%s: %s' % (_module_, _NN, t))

566 ns.append(mod)

567 # check that all other public attrs do exist

568 if attrs and isinstance(attrs, tuple):

569 t = tuple(a for a in attrs if a not in globalocals)

570 if t:

571 s = _Fmt.SQUARE(_s_, len(t)) if len(t) > 1 else _NN

572 t = _COMMASPACE_.join(_DOT_(_pygeodesy_, mod, a) for a in t)

573 raise ImportError('missing %s%s: %s' % (_attribute_, s, t))

574 ns.extend(attrs)

575# XXX if ps: # check that mod is a _pygeodesy_ module

576# XXX m = globalocals[mod] # assert(m.__name__ == mod)

577# XXX f = getattr(m, '__file__', _NN)

578# XXX d = dirname(abspath(f)) if f else pygeodesy_abspath

579# XXX p = getattr(m, '__package__', _NN) or _pygeodesy_

580# XXX if p not in ps or d != pygeodesy_abspath:

581# XXX raise ImportError('foreign module: %s from %r' % (_DOT_(p, mod), f or p))

582 return tuple(set(ns)) # remove duplicates

583

584 __all__ = _all(globals()) # or locals()

585 else:

586 __all__ = ()

587 _init__all__ = False

588

589 from pygeodesy.interns import _DOT_ # PYCHOK import

590__version__ = '23.12.02'

591# see setup.py for similar logic

592 version = _DOT_(*map(int, __version__.split(_DOT_)))

593

594 del abspath, basename, dirname, _DOT_, _lazy_import2, sys

595

596# **) MIT License

597#

598# Copyright (C) 2016-2023 -- mrJean1 at Gmail -- All Rights Reserved.

599#

600# Permission is hereby granted, free of charge, to any person obtaining a

601# copy of this software and associated documentation files (the "Software"),

602# to deal in the Software without restriction, including without limitation

603# the rights to use, copy, modify, merge, publish, distribute, sublicense,

604# and/or sell copies of the Software, and to permit persons to whom the

605# Software is furnished to do so, subject to the following conditions:

606#

607# The above copyright notice and this permission notice shall be included

608# in all copies or substantial portions of the Software.

609#

610# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

611# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

612# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

613# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

614# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

615# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

616# OTHER DEALINGS IN THE SOFTWARE.