1

2# -*- coding: utf-8 -*-

3

4 u'''I{Geocentric} Earth-Centered, Earth-Fixed (ECEF) coordinates.

5

6 Geocentric conversions transcoded from I{Charles Karney}'s C++ class U{Geocentric

7<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1Geocentric.html>}

8 into pure Python class L{EcefKarney}, class L{EcefSudano} based on I{John Sudano}'s

9 U{paper<https://www.ResearchGate.net/publication/

10 3709199_An_exact_conversion_from_an_Earth-centered_coordinate_system_to_latitude_longitude_and_altitude>},

11 class L{EcefVeness} transcoded from I{Chris Veness}' JavaScript classes U{LatLonEllipsoidal,

12 Cartesian<https://www.Movable-Type.co.UK/scripts/geodesy/docs/latlon-ellipsoidal.js.html>}, class L{EcefYou}

13 implementing I{Rey-Jer You}'s U{transformations<https://www.ResearchGate.net/publication/240359424>} and

14 classes L{EcefFarrell22} and L{EcefFarrell22} from I{Jay A. Farrell}'s U{Table 2.1 and 2.2

15<https://Books.Google.com/books?id=fW4foWASY6wC>}, page 29-30.

16

17 Following is a copy of I{Karney}'s U{Detailed Description

18<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1Geocentric.html>}.

19

20 Convert between geodetic coordinates C{lat}-, C{lon}gitude and height C{h} (measured vertically

21 from the surface of the ellipsoid) to geocentric C{x}, C{y} and C{z} coordinates, also known as

22 I{Earth-Centered, Earth-Fixed} (U{ECEF<https://WikiPedia.org/wiki/ECEF>}).

23

24 The origin of geocentric coordinates is at the center of the earth. The C{z} axis goes thru

25 the North pole, C{lat} = 90°. The C{x} axis goes thru C{lat} = 0°, C{lon} = 0°.

26

27 The I{local (cartesian) origin} is at (C{lat0}, C{lon0}, C{height0}). The I{local} C{x} axis points

28 East, the I{local} C{y} axis points North and the I{local} C{z} axis is normal to the ellipsoid. The

29 plane C{z = -height0} is tangent to the ellipsoid, hence the alternate name I{local tangent plane}.

30

31 Forward conversion from geodetic to geocentric (ECEF) coordinates is straightforward.

32

33 For the reverse transformation we use Hugues Vermeille's U{I{Direct transformation from geocentric

34 coordinates to geodetic coordinates}<https://DOI.org/10.1007/s00190-002-0273-6>}, J. Geodesy

35(2002) 76, page 451-454.

36

37 Several changes have been made to ensure that the method returns accurate results for all finite

38 inputs (even if h is infinite). The changes are described in Appendix B of C. F. F. Karney

39 U{I{Geodesics on an ellipsoid of revolution}<https://ArXiv.org/abs/1102.1215v1>}, Feb. 2011, 85,

40 105-117 (U{preprint<https://ArXiv.org/abs/1102.1215v1>}). Vermeille similarly updated his method

41 in U{I{An analytical method to transform geocentric into geodetic coordinates}

42<https://DOI.org/10.1007/s00190-010-0419-x>}, J. Geodesy (2011) 85, page 105-117. See U{Geocentric

43 coordinates<https://GeographicLib.SourceForge.io/C++/doc/geocentric.html>} for more information.

44

45 The errors in these routines are close to round-off. Specifically, for points within 5,000 Km of

46 the surface of the ellipsoid (either inside or outside the ellipsoid), the error is bounded by 7

47 nm (7 nanometers) for the WGS84 ellipsoid. See U{Geocentric coordinates

48<https://GeographicLib.SourceForge.io/C++/doc/geocentric.html>} for further information on the errors.

49

50@note: The C{reverse} methods of all C{Ecef...} classes return by default C{INT0} as the (geodetic)

51 longitude for I{polar} ECEF location C{x == y == 0}. Use keyword argument C{lon00} or property

52 C{lon00} to configure that value.

53

54@see: Module L{ltp} and class L{LocalCartesian}, a transcription of I{Charles Karney}'s C++ class

55 U{LocalCartesian<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1LocalCartesian.html>},

56 for conversion between geodetic and I{local cartesian} coordinates in a I{local tangent

57 plane} as opposed to I{geocentric} (ECEF) ones.

58'''

59

60 from pygeodesy.basics import copysign0, isscalar, issubclassof, neg, map1, \

61 _xinstanceof, _xsubclassof

62 from pygeodesy.constants import EPS, EPS0, EPS02, EPS1, EPS2, EPS_2, INT0, PI, PI_2, \

63 _0_0, _0_0001, _0_01, _0_5, _1_0, _1_0_1T, _N_1_0, \

64 _2_0, _N_2_0, _3_0, _4_0, _6_0, _60_0, _90_0, _N_90_0, \

65 _100_0, _copysign_1_0, isnon0 # PYCHOK used!

66 from pygeodesy.datums import a_f2Tuple, _ellipsoidal_datum, _WGS84, _EWGS84

67# from pygeodesy.ellipsoids import a_f2Tuple, _EWGS84 # from .datums

68 from pygeodesy.errors import _IndexError, LenError, _ValueError, _TypesError, \

69 _xattr, _xdatum, _xkwds, _xkwds_get

70 from pygeodesy.fmath import cbrt, fdot, hypot, hypot1, hypot2_

71 from pygeodesy.fsums import Fsum, fsumf_, Fmt, unstr

72 from pygeodesy.interns import NN, _a_, _C_, _datum_, _ellipsoid_, _f_, _height_, \

73 _lat_, _lon_, _M_, _name_, _singular_, _SPACE_, \

74 _x_, _xyz_, _y_, _z_

75 from pygeodesy.lazily import _ALL_DOCS, _ALL_LAZY, _ALL_MODS as _MODS

76 from pygeodesy.named import _NamedBase, _NamedTuple, notOverloaded, _Pass, _xnamed

77 from pygeodesy.namedTuples import LatLon2Tuple, LatLon3Tuple, \

78 PhiLam2Tuple, Vector3Tuple, Vector4Tuple

79 from pygeodesy.props import deprecated_method, Property_RO, property_RO, property_doc_

80# from pygeodesy.streprs import Fmt, unstr # from .fsums

81 from pygeodesy.units import _isRadius, Degrees, Height, Int, Lam, Lat, Lon, Meter, \

82 Phi, Scalar, Scalar_

83 from pygeodesy.utily import atan1, atan1d, atan2d, degrees90, degrees180, \

84 sincos2, sincos2_, sincos2d, sincos2d_

85

86 from math import atan2, cos, degrees, fabs, radians, sqrt

87

88__all__ = _ALL_LAZY.ecef

89__version__ = '23.12.18'

90

91_Ecef_ = 'Ecef'

92_prolate_ = 'prolate'

93_TRIPS = 33 # 8..9 sufficient, EcefSudano.reverse

94_xyz_y_z = _xyz_, _y_, _z_ # _xargs_kwds_names(_xyzn4)[:3]

95

96

97 class EcefError(_ValueError):

98 '''An ECEF or C{Ecef*} related issue.

99 '''

100 pass

101

102

103 class _EcefBase(_NamedBase):

104 '''(INTERNAL) Base class for L{EcefFarrell21}, L{EcefFarrell22}, L{EcefKarney},

105 L{EcefSudano}, L{EcefVeness} and L{EcefYou}.

106 '''

107 _datum = _WGS84

108 _E = _EWGS84

109 _lon00 = INT0 # arbitrary, "polar" lon for LocalCartesian, Ltp

110

111 def __init__(self, a_ellipsoid=_EWGS84, f=None, name=NN, lon00=INT0):

112 '''New C{Ecef*} converter.

113

114 @arg a_ellipsoid: A (non-prolate) ellipsoid (L{Ellipsoid}, L{Ellipsoid2},

115 L{Datum} or L{a_f2Tuple}) or C{scalar} ellipsoid's

116 equatorial radius (C{meter}).

117 @kwarg f: C{None} or the ellipsoid flattening (C{scalar}), required

118 for C{scalar} B{C{a_ellipsoid}}, C{B{f}=0} represents a

119 sphere, negative B{C{f}} a prolate ellipsoid.

120 @kwarg name: Optional name (C{str}).

121 @kwarg lon00: An arbitrary, I{"polar"} longitude (C{degrees}), see the

122 methods C{reverse}.

123

124 @raise EcefError: If B{C{a_ellipsoid}} not L{Ellipsoid}, L{Ellipsoid2},

125 L{Datum} or L{a_f2Tuple} or C{scalar} or B{C{f}} not

126 C{scalar} or if C{scalar} B{C{a_ellipsoid}} not positive

127 or B{C{f}} not less than 1.0.

128 '''

129 try:

130 E = a_ellipsoid

131 if f is None:

132 pass

133 elif _isRadius(E) and isscalar(f):

134 E = a_f2Tuple(E, f)

135 else:

136 raise ValueError # _invalid_

137

138 if E not in (_EWGS84, _WGS84):

139 d = _ellipsoidal_datum(E, name=name)

140 E = d.ellipsoid

141 if E.a < EPS or E.f > EPS1:

142 raise ValueError # _invalid_

143 self._datum = d

144 self._E = E

145

146 except (TypeError, ValueError) as x:

147 t = unstr(self.classname, a=a_ellipsoid, f=f)

148 raise EcefError(_SPACE_(t, _ellipsoid_), cause=x)

149

150 if name:

151 self.name = name

152 if lon00 is not INT0:

153 self.lon00 = lon00

154

155 def __eq__(self, other):

156 '''Compare this and an other Ecef.

157

158 @arg other: The other ecef (C{Ecef*}).

159

160 @return: C{True} if equal, C{False} otherwise.

161 '''

162 return other is self or (isinstance(other, self.__class__) and

163 other.ellipsoid == self.ellipsoid)

164

165 @Property_RO

166 def datum(self):

167 '''Get the datum (L{Datum}).

168 '''

169 return self._datum

170

171 @Property_RO

172 def ellipsoid(self):

173 '''Get the ellipsoid (L{Ellipsoid} or L{Ellipsoid2}).

174 '''

175 return self._E

176

177 @Property_RO

178 def equatoradius(self):

179 '''Get the C{ellipsoid}'s equatorial radius, semi-axis (C{meter}).

180 '''

181 return self.ellipsoid.a

182

183 a = equatorialRadius = equatoradius # Karney property

184

185 @Property_RO

186 def flattening(self): # Karney property

187 '''Get the C{ellipsoid}'s flattening (C{scalar}), positive for

188 I{oblate}, negative for I{prolate} or C{0} for I{near-spherical}.

189 '''

190 return self.ellipsoid.f

191

192 f = flattening

193

194 def _forward(self, lat, lon, h, name, M=False, _philam=False): # in .ltp.LocalCartesian.forward and -.reset

195 '''(INTERNAL) Common for all C{Ecef*}.

196 '''

197 if _philam: # lat, lon in radians

198 sa, ca, sb, cb = sincos2_(lat, lon)

199 lat = Lat(degrees90( lat), Error=EcefError)

200 lon = Lon(degrees180(lon), Error=EcefError)

201 else:

202 sa, ca, sb, cb = sincos2d_(lat, lon)

203

204 E = self.ellipsoid

205 n = E.roc1_(sa, ca) if self._isYou else E.roc1_(sa)

206 z = (h + n * E.e21) * sa

207 x = (h + n) * ca

208

209 m = self._Matrix(sa, ca, sb, cb) if M else None

210 return Ecef9Tuple(x * cb, x * sb, z, lat, lon, h,

211 0, m, self.datum,

212 name=name or self.name)

213

214 def forward(self, latlonh, lon=None, height=0, M=False, name=NN):

215 '''Convert from geodetic C{(lat, lon, height)} to geocentric C{(x, y, z)}.

216

217 @arg latlonh: Either a C{LatLon}, an L{Ecef9Tuple} or C{scalar}

218 latitude (C{degrees}).

219 @kwarg lon: Optional C{scalar} longitude for C{scalar} B{C{latlonh}}

220 (C{degrees}).

221 @kwarg height: Optional height (C{meter}), vertically above (or below)

222 the surface of the ellipsoid.

223 @kwarg M: Optionally, return the rotation L{EcefMatrix} (C{bool}).

224 @kwarg name: Optional name (C{str}).

225

226 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

227 geocentric C{(x, y, z)} coordinates for the given geodetic ones

228 C{(lat, lon, height)}, case C{C} 0, optional C{M} (L{EcefMatrix})

229 and C{datum} if available.

230

231 @raise EcefError: If B{C{latlonh}} not C{LatLon}, L{Ecef9Tuple} or

232 C{scalar} or B{C{lon}} not C{scalar} for C{scalar}

233 B{C{latlonh}} or C{abs(lat)} exceeds 90°.

234

235 @note: Use method C{.forward_} to specify C{lat} and C{lon} in C{radians}

236 and avoid double angle conversions.

237 '''

238 llhn = _llhn4(latlonh, lon, height, name=name)

239 return self._forward(*llhn, M=M)

240

241 def forward_(self, phi, lam, height=0, M=False, name=NN):

242 '''Like method C{.forward} except with geodetic lat- and longitude given

243 in I{radians}.

244

245 @arg phi: Latitude in I{radians} (C{scalar}).

246 @arg lam: Longitude in I{radians} (C{scalar}).

247 @kwarg height: Optional height (C{meter}), vertically above (or below)

248 the surface of the ellipsoid.

249 @kwarg M: Optionally, return the rotation L{EcefMatrix} (C{bool}).

250 @kwarg name: Optional name (C{str}).

251

252 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)}

253 with C{lat} set to C{degrees90(B{phi})} and C{lon} to

254 C{degrees180(B{lam})}.

255

256 @raise EcefError: If B{C{phi}} or B{C{lam}} invalid or not C{scalar}.

257 '''

258 try: # like function C{_llhn4} above

259 plhn = Phi(phi), Lam(lam), Height(height), name

260 except (TypeError, ValueError) as x:

261 raise EcefError(phi=phi, lam=lam, height=height, cause=x)

262 return self._forward(*plhn, M=M, _philam=True)

263

264 @property_RO

265 def _Geocentrics(self):

266 '''(INTERNAL) Get the valid geocentric classes. I{once}.

267 '''

268 _EcefBase._Geocentrics = t = (Ecef9Tuple, # overwrite property_RO

269 _MODS.cartesianBase.CartesianBase)

270 return t

271

272 @Property_RO

273 def _isYou(self):

274 '''(INTERNAL) Is this an C{EcefYou}?.

275 '''

276 return isinstance(self, EcefYou)

277

278 @property

279 def lon00(self):

280 '''Get the I{"polar"} longitude (C{degrees}), see method C{reverse}.

281 '''

282 return self._lon00

283

284 @lon00.setter # PYCHOK setter!

285 def lon00(self, lon00):

286 '''Set the I{"polar"} longitude (C{degrees}), see method C{reverse}.

287 '''

288 self._lon00 = Degrees(lon00=lon00)

289

290 def _Matrix(self, sa, ca, sb, cb):

291 '''Creation a rotation matrix.

292

293 @arg sa: C{sin(phi)} (C{float}).

294 @arg ca: C{cos(phi)} (C{float}).

295 @arg sb: C{sin(lambda)} (C{float}).

296 @arg cb: C{cos(lambda)} (C{float}).

297

298 @return: An L{EcefMatrix}.

299 '''

300 return self._xnamed(EcefMatrix(sa, ca, sb, cb))

301

302 def _polon(self, y, x, R, **name_lon00):

303 '''(INTERNAL) Handle I{"polar"} longitude.

304 '''

305 return atan2d(y, x) if R else _xkwds_get(name_lon00, lon00=self.lon00)

306

307 def reverse(self, xyz, y=None, z=None, M=False, **name_lon00): # PYCHOK no cover

308 '''I{Must be overloaded}.'''

309 notOverloaded(self, xyz, y=y, z=z, M=M, **name_lon00)

310

311 def toStr(self, prec=9, **unused): # PYCHOK signature

312 '''Return this C{Ecef*} as a string.

313

314 @kwarg prec: Precision, number of decimal digits (0..9).

315

316 @return: This C{Ecef*} (C{str}).

317 '''

318 return self.attrs(_a_, _f_, _datum_, _name_, prec=prec) # _ellipsoid_

319

320

321 class EcefFarrell21(_EcefBase):

322 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF)

323 coordinates based on I{Jay A. Farrell}'s U{Table 2.1<https://Books.Google.com/

324 books?id=fW4foWASY6wC>}, page 29.

325 '''

326

327 def reverse(self, xyz, y=None, z=None, M=None, **name_lon00): # PYCHOK unused M

328 '''Convert from geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)} using

329 I{Farrell}'s U{Table 2.1<https://Books.Google.com/books?id=fW4foWASY6wC>},

330 page 29.

331

332 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

333 coordinate (C{meter}).

334 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

335 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

336 @kwarg M: I{Ignored}, rotation matrix C{M} not available.

337 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

338 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

339 the default and property C{lon00} setting and returned if

340 C{B{x}=0} and C{B{y}=0}.

341

342 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

343 geodetic coordinates C{(lat, lon, height)} for the given geocentric

344 ones C{(x, y, z)}, case C{C=1}, C{M=None} always and C{datum}

345 if available.

346

347 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or B{C{z}}

348 not C{scalar} for C{scalar} B{C{xyz}} or C{sqrt} domain or

349 zero division error.

350

351 @see: L{EcefFarrell22} and L{EcefVeness}.

352 '''

353 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

354

355 E = self.ellipsoid

356 a = E.a

357 a2 = E.a2

358 b2 = E.b2

359 e2 = E.e2

360 e2_ = E.e2abs * E.a2_b2 # (E.e * E.a_b)**2 = 0.0820944... WGS84

361 e4 = E.e4

362

363 try: # names as page 29

364 z2 = z**2

365 ez = z2 * (_1_0 - e2) # E.e2s2(z)

366

367 p = hypot(x, y)

368 p2 = p**2

369 G = p2 + ez - e2 * (a2 - b2) # p2 + ez - e4 * a2

370 F = b2 * z2 * 54

371 t = e4 * p2 * F / G**3

372 t = cbrt(sqrt(t * (t + _2_0)) + t + _1_0)

373 G *= fsumf_(t , _1_0, _1_0 / t)

374 P = F / (G**2 * _3_0)

375 Q = sqrt(_2_0 * e4 * P + _1_0)

376 Q1 = Q + _1_0

377 r0 = P * p * e2 / Q1 - sqrt(fsumf_(a2 * (Q1 / Q) * _0_5,

378 -P * ez / (Q * Q1),

379 -P * p2 * _0_5))

380 r = p + e2 * r0

381 v = b2 / (sqrt(r**2 + ez) * a)

382

383 h = hypot(r, z) * (_1_0 - v)

384 lat = atan1d((e2_ * v + _1_0) * z, p)

385 lon = self._polon(y, x, p, **name_lon00)

386 # note, phi and lam are swapped on page 29

387

388 except (ValueError, ZeroDivisionError) as e:

389 raise EcefError(x=x, y=y, z=z, cause=e)

390

391 return Ecef9Tuple(x, y, z, lat, lon, h,

392 1, None, self.datum,

393 name=name or self.name)

394

395

396 class EcefFarrell22(_EcefBase):

397 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF)

398 coordinates based on I{Jay A. Farrell}'s U{Table 2.2<https://Books.Google.com/

399 books?id=fW4foWASY6wC>}, page 30.

400 '''

401

402 def reverse(self, xyz, y=None, z=None, M=None, **name_lon00): # PYCHOK unused M

403 '''Convert from geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)} using

404 I{Farrell}'s U{Table 2.2<https://Books.Google.com/books?id=fW4foWASY6wC>},

405 page 30.

406

407 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

408 coordinate (C{meter}).

409 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

410 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

411 @kwarg M: I{Ignored}, rotation matrix C{M} not available.

412 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

413 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

414 the default and property C{lon00} setting and returned in case

415 C{B{x}=0} and C{B{y}=0}.

416

417 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

418 geodetic coordinates C{(lat, lon, height)} for the given geocentric

419 ones C{(x, y, z)}, case C{C=1}, C{M=None} always and C{datum}

420 if available.

421

422 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or B{C{z}}

423 not C{scalar} for C{scalar} B{C{xyz}} or C{sqrt} domain or

424 zero division error.

425

426 @see: L{EcefFarrell21} and L{EcefVeness}.

427 '''

428 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

429

430 E = self.ellipsoid

431 a = E.a

432 b = E.b

433

434 try: # see EcefVeness.reverse

435 p = hypot(x, y)

436 lon = self._polon(y, x, p, **name_lon00)

437

438 s, c = sincos2(atan2(z * a, p * b)) # == _norm3

439 lat = atan1d(z + s**3 * b * E.e22,

440 p - c**3 * a * E.e2)

441

442 s, c = sincos2d(lat)

443 if c: # E.roc1_(s) = E.a / sqrt(1 - E.e2 * s**2)

444 h = p / c - (E.roc1_(s) if s else a)

445 else: # polar

446 h = fabs(z) - b

447 # note, phi and lam are swapped on page 30

448

449 except (ValueError, ZeroDivisionError) as e:

450 raise EcefError(x=x, y=y, z=z, cause=e)

451

452 return Ecef9Tuple(x, y, z, lat, lon, h,

453 1, None, self.datum,

454 name=name or self.name)

455

456

457 class EcefKarney(_EcefBase):

458 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF)

459 coordinates transcoded from I{Karney}'s C++ U{Geocentric<https://GeographicLib.SourceForge.io/

460 C++/doc/classGeographicLib_1_1Geocentric.html>} methods.

461

462 @note: On methods C{.forward} and C{.forwar_}, let C{v} be a unit vector located

463 at C{(lat, lon, h)}. We can express C{v} as column vectors in one of two

464 ways, C{v1} in East, North, Up (ENU) coordinates (where the components are

465 relative to a local coordinate system at C{C(lat0, lon0, h0)}) or as C{v0}

466 in geocentric C{x, y, z} coordinates. Then, M{v0 = M ⋅ v1} where C{M} is

467 the rotation matrix.

468 '''

469

470 @Property_RO

471 def hmax(self):

472 '''Get the distance or height limit (C{meter}, conventionally).

473 '''

474 return self.equatoradius / EPS_2 # self.equatoradius * _2_EPS, 12M lighyears

475

476 def reverse(self, xyz, y=None, z=None, M=False, **name_lon00):

477 '''Convert from geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)}.

478

479 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

480 coordinate (C{meter}).

481 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

482 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

483 @kwarg M: Optionally, return the rotation L{EcefMatrix} (C{bool}).

484 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

485 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

486 the default and property C{lon00} setting and returned in case

487 C{B{x}=0} and C{B{y}=0}.

488

489 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

490 geodetic coordinates C{(lat, lon, height)} for the given geocentric

491 ones C{(x, y, z)}, case C{C}, optional C{M} (L{EcefMatrix}) and

492 C{datum} if available.

493

494 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or B{C{z}}

495 not C{scalar} for C{scalar} B{C{xyz}}.

496

497 @note: In general, there are multiple solutions and the result which minimizes

498 C{height} is returned, i.e., the C{(lat, lon)} corresponding to the

499 closest point on the ellipsoid. If there are still multiple solutions

500 with different latitudes (applies only if C{z} = 0), then the solution

501 with C{lat} > 0 is returned. If there are still multiple solutions with

502 different longitudes (applies only if C{x} = C{y} = 0), then C{lon00} is

503 returned. The returned C{lon} is in the range [−180°, 180°] and C{height}

504 is not below M{−E.a * (1 − E.e2) / sqrt(1 − E.e2 * sin(lat)**2)}. Like

505 C{forward} above, M{v1 = Transpose(M) ⋅ v0}.

506 '''

507 def _norm3(y, x):

508 h = hypot(y, x) # EPS0, EPS_2

509 return (y / h, x / h, h) if h > 0 else (_0_0, _1_0, h)

510

511 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

512

513 E = self.ellipsoid

514 f = E.f

515

516 sb, cb, R = _norm3(y, x)

517 h = hypot(R, z) # distance to earth center

518 if h > self.hmax: # PYCHOK no cover

519 # We are really far away (> 12M light years). Treat the earth

520 # as a point and h above as an acceptable approximation to the

521 # height. This avoids overflow, e.g., in the computation of d

522 # below. It's possible that h has overflowed to INF, that's OK.

523 # Treat finite x, y, but R overflows to +INF by scaling by 2.

524 sb, cb, R = _norm3(y * _0_5, x * _0_5)

525 sa, ca, _ = _norm3(z * _0_5, R)

526 C = 1

527

528 elif E.e4: # E.isEllipsoidal

529 # Treat prolate spheroids by swapping R and Z here and by

530 # switching the arguments to phi = atan2(...) at the end.

531 p = (R / E.a)**2

532 q = (z / E.a)**2 * E.e21

533 if f < 0:

534 p, q = q, p

535 r = fsumf_(p, q, -E.e4)

536 e = E.e4 * q

537 if e or r > 0:

538 # Avoid possible division by zero when r = 0 by multiplying

539 # equations for s and t by r^3 and r, respectively.

540 s = d = e * p / _4_0 # s = r^3 * s

541 u = r = r / _6_0

542 r2 = r**2

543 r3 = r2 * r

544 t3 = r3 + s

545 d *= t3 + r3

546 if d < 0:

547 # t is complex, but the way u is defined, the result is real.

548 # There are three possible cube roots. We choose the root

549 # which avoids cancellation. Note, d < 0 implies r < 0.

550 u += cos(atan2(sqrt(-d), -t3) / _3_0) * r * _2_0

551 else:

552 # Pick the sign on the sqrt to maximize abs(t3). This

553 # minimizes loss of precision due to cancellation. The

554 # result is unchanged because of the way the t is used

555 # in definition of u.

556 if d > 0:

557 t3 += copysign0(sqrt(d), t3) # t3 = (r * t)^3

558 # N.B. cbrt always returns the real root, cbrt(-8) = -2.

559 t = cbrt(t3) # t = r * t

560 if t: # t can be zero; but then r2 / t -> 0.

561 u = fsumf_(u, t, r2 / t)

562 v = sqrt(e + u**2) # guaranteed positive

563 # Avoid loss of accuracy when u < 0. Underflow doesn't occur in

564 # E.e4 * q / (v - u) because u ~ e^4 when q is small and u < 0.

565 u = (e / (v - u)) if u < 0 else (u + v) # u+v, guaranteed positive

566 # Need to guard against w going negative due to roundoff in u - q.

567 w = E.e2abs * (u - q) / (_2_0 * v)

568 # Rearrange expression for k to avoid loss of accuracy due to

569 # subtraction. Division by 0 not possible because u > 0, w >= 0.

570 k1 = k2 = (u / (sqrt(u + w**2) + w)) if w > 0 else sqrt(u)

571 if f < 0:

572 k1 -= E.e2

573 else:

574 k2 += E.e2

575 sa, ca, h = _norm3(z / k1, R / k2)

576 h *= k1 - E.e21

577 C = 2

578

579 else: # e = E.e4 * q == 0 and r <= 0

580 # This leads to k = 0 (oblate, equatorial plane) and k + E.e^2 = 0

581 # (prolate, rotation axis) and the generation of 0/0 in the general

582 # formulas for phi and h, using the general formula and division

583 # by 0 in formula for h. Handle this case by taking the limits:

584 # f > 0: z -> 0, k -> E.e2 * sqrt(q) / sqrt(E.e4 - p)

585 # f < 0: r -> 0, k + E.e2 -> -E.e2 * sqrt(q) / sqrt(E.e4 - p)

586 q = E.e4 - p

587 if f < 0:

588 p, q = q, p

589 e = E.a

590 else:

591 e = E.b2_a

592 sa, ca, h = _norm3(sqrt(q * E._1_e21), sqrt(p))

593 if z < 0: # for tiny negative z, not for prolate

594 sa = neg(sa)

595 h *= neg(e / E.e2abs)

596 C = 3

597

598 else: # E.e4 == 0, spherical case

599 # Dealing with underflow in the general case with E.e2 = 0 is

600 # difficult. Origin maps to North pole, same as with ellipsoid.

601 sa, ca, _ = _norm3((z if h else _1_0), R)

602 h -= E.a

603 C = 4

604

605 # lon00 <https://GitHub.com/mrJean1/PyGeodesy/issues/77>

606 lon = self._polon(sb, cb, R, **name_lon00)

607 m = self._Matrix(sa, ca, sb, cb) if M else None

608 return Ecef9Tuple(x, y, z, atan1d(sa, ca), lon, h,

609 C, m, self.datum,

610 name=name or self.name)

611

612

613 class EcefSudano(_EcefBase):

614 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF) coordinates

615 based on I{John J. Sudano}'s U{paper<https://www.ResearchGate.net/publication/3709199>}.

616 '''

617 _tol = EPS2

618

619 def reverse(self, xyz, y=None, z=None, M=None, **name_lon00): # PYCHOK unused M

620 '''Convert from geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)} using

621 I{Sudano}'s U{iterative method<https://www.ResearchGate.net/publication/3709199>}.

622

623 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

624 coordinate (C{meter}).

625 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

626 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

627 @kwarg M: I{Ignored}, rotation matrix C{M} not available.

628 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

629 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

630 the default and property C{lon00} setting and returned in case

631 C{B{x}=0} and C{B{y}=0}.

632

633 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with geodetic

634 coordinates C{(lat, lon, height)} for the given geocentric ones C{(x, y, z)},

635 iteration C{C}, C{M=None} always and C{datum} if available.

636

637 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or B{C{z}}

638 not C{scalar} for C{scalar} B{C{xyz}} or no convergence.

639 '''

640 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

641

642 E = self.ellipsoid

643 e = E.e2 * E.a

644 R = hypot(x, y) # Rh

645 d = e - R

646

647 _a = fabs

648 lat = atan1d(z, R * E.e21)

649 sa, ca = sincos2d(fabs(lat))

650 # Sudano's Eq (A-6) and (A-7) refactored/reduced,

651 # replacing Rn from Eq (A-4) with n = E.a / ca:

652 # N = ca**2 * ((z + E.e2 * n * sa) * ca - R * sa)

653 # = ca**2 * (z * ca + E.e2 * E.a * sa - R * sa)

654 # = ca**2 * (z * ca + (E.e2 * E.a - R) * sa)

655 # D = ca**3 * (E.e2 * n / E.e2s2(sa)) - R

656 # = ca**2 * (E.e2 * E.a / E.e2s2(sa) - R / ca**2)

657 # N / D = (z * ca + (E.e2 * E.a - R) * sa) /

658 # (E.e2 * E.a / E.e2s2(sa) - R / ca**2)

659 tol = self.tolerance

660 _S2 = Fsum(sa).fsum2_

661 _rt = sqrt

662 for i in range(1, _TRIPS):

663 ca2 = _1_0 - sa**2

664 if ca2 < EPS_2: # PYCHOK no cover

665 ca = _0_0

666 break

667 ca = _rt(ca2)

668 r = e / E.e2s2(sa) - R / ca2

669 if _a(r) < EPS_2:

670 break

671 lat = None

672 sa, r = _S2(-z * ca / r, -d * sa / r)

673 if _a(r) < tol:

674 break

675 else:

676 t = unstr(self.reverse, x=x, y=y, z=z)

677 raise EcefError(t, txt=Fmt.no_convergence(r, tol))

678

679 if lat is None:

680 lat = copysign0(atan1d(_a(sa), ca), z)

681 lon = self._polon(y, x, R, **name_lon00)

682

683 h = fsumf_(R * ca, _a(z * sa), -E.a * E.e2s(sa)) # use Veness'

684 # because Sudano's Eq (7) doesn't produce the correct height

685 # h = (fabs(z) + R - E.a * cos(a + E.e21) * sa / ca) / (ca + sa)

686 return Ecef9Tuple(x, y, z, lat, lon, h,

687 i, None, self.datum, # C=i, M=None

688 iteration=i, name=name or self.name)

689

690 @property_doc_(''' the convergence tolerance (C{float}).''')

691 def tolerance(self):

692 '''Get the convergence tolerance (C{scalar}).

693 '''

694 return self._tol

695

696 @tolerance.setter # PYCHOK setter!

697 def tolerance(self, tol):

698 '''Set the convergence tolerance (C{scalar}).

699

700 @raise EcefError: Non-scalar or invalid B{C{tol}}.

701 '''

702 self._tol = Scalar_(tolerance=tol, low=EPS, Error=EcefError)

703

704

705 class EcefVeness(_EcefBase):

706 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF) coordinates

707 transcoded from I{Chris Veness}' JavaScript classes U{LatLonEllipsoidal, Cartesian<https://

708 www.Movable-Type.co.UK/scripts/geodesy/docs/latlon-ellipsoidal.js.html>}.

709

710 @see: U{I{A Guide to Coordinate Systems in Great Britain}<https://www.OrdnanceSurvey.co.UK/

711 documents/resources/guide-coordinate-systems-great-britain.pdf>}, section I{B) Converting

712 between 3D Cartesian and ellipsoidal latitude, longitude and height coordinates}.

713 '''

714

715 def reverse(self, xyz, y=None, z=None, M=None, **name_lon00): # PYCHOK unused M

716 '''Conversion from geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)}

717 transcoded from I{Chris Veness}' U{JavaScript<https://www.Movable-Type.co.UK/

718 scripts/geodesy/docs/latlon-ellipsoidal.js.html>}.

719

720 Uses B. R. Bowring’s formulation for μm precision in concise form U{I{The accuracy

721 of geodetic latitude and height equations}<https://www.ResearchGate.net/publication/

722 233668213>}, Survey Review, Vol 28, 218, Oct 1985.

723

724 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

725 coordinate (C{meter}).

726 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

727 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

728 @kwarg M: I{Ignored}, rotation matrix C{M} not available.

729 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

730 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

731 the default and property C{lon00} setting and returned in case

732 C{B{x}=0} and C{B{y}=0}.

733

734 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

735 geodetic coordinates C{(lat, lon, height)} for the given geocentric

736 ones C{(x, y, z)}, case C{C}, C{M=None} always and C{datum} if available.

737

738 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or B{C{z}}

739 not C{scalar} for C{scalar} B{C{xyz}}.

740

741 @see: Toms, Ralph M. U{I{An Efficient Algorithm for Geocentric to Geodetic

742 Coordinate Conversion}<https://www.OSTI.gov/scitech/biblio/110235>},

743 Sept 1995 and U{I{An Improved Algorithm for Geocentric to Geodetic

744 Coordinate Conversion}<https://www.OSTI.gov/scitech/servlets/purl/231228>},

745 Apr 1996, both from Lawrence Livermore National Laboratory (LLNL) and

746 Sudano, John J, U{I{An exact conversion from an Earth-centered coordinate

747 system to latitude longitude and altitude}<https://www.ResearchGate.net/

748 publication/3709199>}.

749 '''

750 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

751

752 E = self.ellipsoid

753 a = E.a

754

755 p = hypot(x, y) # distance from minor axis

756 r = hypot(p, z) # polar radius

757 if min(p, r) > EPS0:

758 b = E.b * E.e22

759 # parametric latitude (Bowring eqn 17, replaced)

760 t = (E.b * z) / (a * p) * (_1_0 + b / r)

761 c = _1_0 / hypot1(t)

762 s = c * t

763 # geodetic latitude (Bowring eqn 18)

764 lat = atan1d(z + s**3 * b,

765 p - c**3 * a * E.e2)

766

767 # height above ellipsoid (Bowring eqn 7)

768 sa, ca = sincos2d(lat)

769# r = a / E.e2s(sa) # length of normal terminated by minor axis

770# h = p * ca + z * sa - (a * a / r)

771 h = fsumf_(p * ca, z * sa, -a * E.e2s(sa))

772 C = 1

773

774 # see <https://GIS.StackExchange.com/questions/28446>

775 elif p > EPS: # lat arbitrarily zero, equatorial lon

776 C, lat, h = 2, _0_0, (p - a)

777

778 else: # polar lat, lon arbitrarily lon00

779 C, lat, h = 3, (_N_90_0 if z < 0 else _90_0), (fabs(z) - E.b)

780

781 lon = self._polon(y, x, p, **name_lon00)

782 return Ecef9Tuple(x, y, z, lat, lon, h,

783 C, None, self.datum, # M=None

784 name=name or self.name)

785

786

787 class EcefYou(_EcefBase):

788 '''Conversion between geodetic and geocentric, I{Earth-Centered, Earth-Fixed} (ECEF) coordinates

789 using I{Rey-Jer You}'s U{transformation<https://www.ResearchGate.net/publication/240359424>}

790 for I{non-prolate} ellipsoids.

791

792 @see: Featherstone, W.E., Claessens, S.J. U{I{Closed-form transformation between geodetic and

793 ellipsoidal coordinates}<https://Espace.Curtin.edu.AU/bitstream/handle/20.500.11937/

794 11589/115114_9021_geod2ellip_final.pdf>} Studia Geophysica et Geodaetica, 2008, 52,

795 pages 1-18 and U{PyMap3D <https://PyPI.org/project/pymap3d>}.

796 '''

797

798 def __init__(self, a_ellipsoid=_EWGS84, f=None, **name_lon00): # PYCHOK signature

799 _EcefBase.__init__(self, a_ellipsoid, f=f, **name_lon00) # inherited documentation

800 _ = EcefYou._e2(self.ellipsoid)

801

802 @staticmethod

803 def _e2(E):

804 e2 = E.a2 - E.b2

805 if e2 < 0 or E.f < 0:

806 raise EcefError(ellipsoid=E, txt=_prolate_)

807 return e2

808

809 def reverse(self, xyz, y=None, z=None, M=None, **name_lon00): # PYCHOK unused M

810 '''Convert geocentric C{(x, y, z)} to geodetic C{(lat, lon, height)}

811 using I{Rey-Jer You}'s transformation.

812

813 @arg xyz: A geocentric (C{Cartesian}, L{Ecef9Tuple}) or C{scalar} ECEF C{x}

814 coordinate (C{meter}).

815 @kwarg y: ECEF C{y} coordinate for C{scalar} B{C{xyz}} and B{C{z}} (C{meter}).

816 @kwarg z: ECEF C{z} coordinate for C{scalar} B{C{xyz}} and B{C{y}} (C{meter}).

817 @kwarg M: I{Ignored}, rotation matrix C{M} not available.

818 @kwarg name_lon00: Optional keyword arguments C{B{name}=NN} (C{str}) and

819 I{"polar"} longitude C{B{lon00}=INT0} (C{degrees}), overriding

820 the default and property C{lon00} setting and returned in case

821 C{B{x}=0} and C{B{y}=0}.

822

823 @return: An L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with

824 geodetic coordinates C{(lat, lon, height)} for the given geocentric

825 ones C{(x, y, z)}, case C{C=1}, C{M=None} always and C{datum} if

826 available.

827

828 @raise EcefError: Invalid B{C{xyz}} or C{scalar} C{x} or B{C{y}} and/or

829 B{C{z}} not C{scalar} for C{scalar} B{C{xyz}} or the

830 ellipsoid is I{prolate}.

831 '''

832 x, y, z, name = _xyzn4(xyz, y, z, self._Geocentrics, **name_lon00)

833

834 E = self.ellipsoid

835 e2 = EcefYou._e2(E)

836 e = sqrt(e2) if e2 > 0 else _0_0 # XXX sqrt0(e2)?

837

838 q = hypot( x, y) # R

839 r2 = hypot2_(x, y, z)

840 u = fsumf_(r2, -e2, hypot(r2 - e2, e * z * _2_0)) * _0_5

841 if u > EPS02:

842 u = sqrt(u)

843 p = hypot(u, e)

844 B = atan1(p * z, u * q) # beta0 = atan(p / u * z / q)

845 sB, cB = sincos2(B)

846 if cB and sB:

847 p *= E.a

848 d = (p / cB - e2 * cB) / sB

849 if isnon0(d):

850 B += fsumf_(u * E.b, -p, e2) / d

851 sB, cB = sincos2(B)

852 elif u < 0:

853 raise EcefError(x=x, y=y, z=z, txt=_singular_)

854 else:

855 sB, cB = _copysign_1_0(z), _0_0

856

857 lat = atan1d(E.a * sB, E.b * cB) # atan(E.a_b * tan(B))

858 lon = self._polon(y, x, q, **name_lon00)

859

860 h = hypot(z - E.b * sB, q - E.a * cB)

861 if hypot2_(x, y, z * E.a_b) < E.a2:

862 h = neg(h) # inside ellipsoid

863 return Ecef9Tuple(x, y, z, lat, lon, h,

864 1, None, self.datum, # C=1, M=None

865 name=name or self.name)

866

867

868 class EcefMatrix(_NamedTuple):

869 '''A rotation matrix known as I{East-North-Up (ENU) to ECEF}.

870

871 @see: U{From ENU to ECEF<https://WikiPedia.org/wiki/

872 Geographic_coordinate_conversion#From_ECEF_to_ENU>} and

873 U{Issue #74<https://Github.com/mrJean1/PyGeodesy/issues/74>}.

874 '''

875 _Names_ = ('_0_0_', '_0_1_', '_0_2_', # row-order

876 '_1_0_', '_1_1_', '_1_2_',

877 '_2_0_', '_2_1_', '_2_2_')

878 _Units_ = (Scalar,) * len(_Names_)

879

880 def _validate(self, **_OK): # PYCHOK unused

881 '''(INTERNAL) Allow C{_Names_} with leading underscore.

882 '''

883 _NamedTuple._validate(self, _OK=True)

884

885 def __new__(cls, sa, ca, sb, cb, *_more):

886 '''New L{EcefMatrix} matrix.

887

888 @arg sa: C{sin(phi)} (C{float}).

889 @arg ca: C{cos(phi)} (C{float}).

890 @arg sb: C{sin(lambda)} (C{float}).

891 @arg cb: C{cos(lambda)} (C{float}).

892 @arg _more: (INTERNAL) from C{.multiply}.

893

894 @raise EcefError: If B{C{sa}}, B{C{ca}}, B{C{sb}} or

895 B{C{cb}} outside M{[-1.0, +1.0]}.

896 '''

897 t = sa, ca, sb, cb

898 if _more: # all 9 matrix elements ...

899 t += _more # ... from .multiply

900

901 elif max(map(fabs, t)) > _1_0:

902 raise EcefError(unstr(EcefMatrix.__name__, *t))

903

904 else: # build matrix from the following quaternion operations

905 # qrot(lam, [0,0,1]) * qrot(phi, [0,-1,0]) * [1,1,1,1]/2

906 # or

907 # qrot(pi/2 + lam, [0,0,1]) * qrot(-pi/2 + phi, [-1,0,0])

908 # where

909 # qrot(t,v) = [cos(t/2), sin(t/2)*v[1], sin(t/2)*v[2], sin(t/2)*v[3]]

910

911 # Local X axis (East) in geocentric coords

912 # M[0] = -slam; M[3] = clam; M[6] = 0;

913 # Local Y axis (North) in geocentric coords

914 # M[1] = -clam * sphi; M[4] = -slam * sphi; M[7] = cphi;

915 # Local Z axis (Up) in geocentric coords

916 # M[2] = clam * cphi; M[5] = slam * cphi; M[8] = sphi;

917 t = (-sb, -cb * sa, cb * ca,

918 cb, -sb * sa, sb * ca,

919 _0_0, ca, sa)

920

921 return _NamedTuple.__new__(cls, *t)

922

923 def column(self, column):

924 '''Get this matrix' B{C{column}} 0, 1 or 2 as C{3-tuple}.

925 '''

926 if 0 <= column < 3:

927 return self[column::3]

928 raise _IndexError(column=column)

929

930 def copy(self, **unused): # PYCHOK signature

931 '''Make a shallow or deep copy of this instance.

932

933 @return: The copy (C{This class} or subclass thereof).

934 '''

935 return self.classof(*self)

936

937 __copy__ = __deepcopy__ = copy

938

939 @Property_RO

940 def matrix3(self):

941 '''Get this matrix' rows (C{3-tuple} of 3 C{3-tuple}s).

942 '''

943 return tuple(map(self.row, range(3)))

944

945 @Property_RO

946 def matrixTransposed3(self):

947 '''Get this matrix' I{Transposed} rows (C{3-tuple} of 3 C{3-tuple}s).

948 '''

949 return tuple(map(self.column, range(3)))

950

951 def multiply(self, other):

952 '''Matrix multiply M{M0' ⋅ M} this matrix I{Transposed}

953 with an other matrix.

954

955 @arg other: The other matrix (L{EcefMatrix}).

956

957 @return: The matrix product (L{EcefMatrix}).

958

959 @raise TypeError: If B{C{other}} is not L{EcefMatrix}.

960 '''

961 _xinstanceof(EcefMatrix, other=other)

962 # like LocalCartesian.MatrixMultiply, C{self.matrixTransposed3 X other.matrix3}

963 # <https://GeographicLib.SourceForge.io/C++/doc/LocalCartesian_8cpp_source.html>

964 # X = (fdot(self.column(r), *other.column(c)) for r in (0,1,2) for c in (0,1,2))

965 X = (fdot(self[r::3], *other[c::3]) for r in range(3) for c in range(3))

966 return _xnamed(EcefMatrix(*X), EcefMatrix.multiply.__name__)

967

968 def rotate(self, xyz, *xyz0):

969 '''Forward rotation M{M0' ⋅ ([x, y, z] - [x0, y0, z0])'}.

970

971 @arg xyz: Local C{(x, y, z)} coordinates (C{3-tuple}).

972 @arg xyz0: Optional, local C{(x0, y0, z0)} origin (C{3-tuple}).

973

974 @return: Rotated C{(x, y, z)} location (C{3-tuple}).

975

976 @raise LenError: Unequal C{len(B{xyz})} and C{len(B{xyz0})}.

977 '''

978 if xyz0:

979 if len(xyz0) != len(xyz):

980 raise LenError(self.rotate, xyz0=len(xyz0), xyz=len(xyz))

981 xyz = tuple(c - c0 for c, c0 in zip(xyz, xyz0))

982

983 # x' = M[0] * x + M[3] * y + M[6] * z

984 # y' = M[1] * x + M[4] * y + M[7] * z

985 # z' = M[2] * x + M[5] * y + M[8] * z

986 return (fdot(xyz, *self[0::3]), # .column(0)

987 fdot(xyz, *self[1::3]), # .column(1)

988 fdot(xyz, *self[2::3])) # .column(2)

989

990 def row(self, row):

991 '''Get this matrix' B{C{row}} 0, 1 or 2 as C{3-tuple}.

992 '''

993 if 0 <= row < 3:

994 r = row * 3

995 return self[r: r+3]

996 raise _IndexError(row=row)

997

998 def unrotate(self, xyz, *xyz0):

999 '''Inverse rotation M{[x0, y0, z0] + M0 ⋅ [x,y,z]'}.

1000

1001 @arg xyz: Local C{(x, y, z)} coordinates (C{3-tuple}).

1002 @arg xyz0: Optional, local C{(x0, y0, z0)} origin (C{3-tuple}).

1003

1004 @return: Unrotated C{(x, y, z)} location (C{3-tuple}).

1005

1006 @raise LenError: Unequal C{len(B{xyz})} and C{len(B{xyz0})}.

1007 '''

1008 if xyz0:

1009 if len(xyz0) != len(xyz):

1010 raise LenError(self.unrotate, xyz0=len(xyz0), xyz=len(xyz))

1011 _xyz = _1_0_1T + xyz

1012 # x' = x0 + M[0] * x + M[1] * y + M[2] * z

1013 # y' = y0 + M[3] * x + M[4] * y + M[5] * z

1014 # z' = z0 + M[6] * x + M[7] * y + M[8] * z

1015 xyz_ = (fdot(_xyz, xyz0[0], *self[0:3]), # .row(0)

1016 fdot(_xyz, xyz0[1], *self[3:6]), # .row(1)

1017 fdot(_xyz, xyz0[2], *self[6:9])) # .row(2)

1018 else:

1019 # x' = M[0] * x + M[1] * y + M[2] * z

1020 # y' = M[3] * x + M[4] * y + M[5] * z

1021 # z' = M[6] * x + M[7] * y + M[8] * z

1022 xyz_ = (fdot(xyz, *self[0:3]), # .row(0)

1023 fdot(xyz, *self[3:6]), # .row(1)

1024 fdot(xyz, *self[6:9])) # .row(2)

1025 return xyz_

1026

1027

1028 class Ecef9Tuple(_NamedTuple):

1029 '''9-Tuple C{(x, y, z, lat, lon, height, C, M, datum)} with I{geocentric}

1030 C{x}, C{y} and C{z} plus I{geodetic} C{lat}, C{lon} and C{height}, case

1031 C{C} (see the C{Ecef*.reverse} methods) and optionally, the rotation

1032 matrix C{M} (L{EcefMatrix}) and C{datum}, with C{lat} and C{lon} in

1033 C{degrees} and C{x}, C{y}, C{z} and C{height} in C{meter}, conventionally.

1034 '''

1035 _Names_ = (_x_, _y_, _z_, _lat_, _lon_, _height_, _C_, _M_, _datum_)

1036 _Units_ = ( Meter, Meter, Meter, Lat, Lon, Height, Int, _Pass, _Pass)

1037

1038 @property_RO

1039 def _CartesianBase(self):

1040 '''(INTERNAL) Get class C{CartesianBase}, I{once}.

1041 '''

1042 Ecef9Tuple._CartesianBase = C = _MODS.cartesianBase.CartesianBase # overwrite property_RO

1043 return C

1044

1045 @deprecated_method

1046 def convertDatum(self, datum2): # for backward compatibility

1047 '''DEPRECATED, use method L{toDatum}.'''

1048 return self.toDatum(datum2)

1049

1050 @Property_RO

1051 def lam(self):

1052 '''Get the longitude in C{radians} (C{float}).

1053 '''

1054 return self.philam.lam

1055

1056 @Property_RO

1057 def lamVermeille(self):

1058 '''Get the longitude in C{radians} M{[-PI*3/2..+PI*3/2]} after U{Vermeille

1059 <https://Search.ProQuest.com/docview/639493848>} (2004), page 95.

1060

1061 @see: U{Karney<https://GeographicLib.SourceForge.io/C++/doc/geocentric.html>},

1062 U{Vermeille<https://Search.ProQuest.com/docview/847292978>} 2011, pp 112-113, 116

1063 and U{Featherstone, et.al.<https://Search.ProQuest.com/docview/872827242>}, page 7.

1064 '''

1065 x, y = self.x, self.y

1066 if y > EPS0:

1067 r = atan2(x, hypot(y, x) + y) * _N_2_0 + PI_2

1068 elif y < -EPS0:

1069 r = atan2(x, hypot(y, x) - y) * _2_0 - PI_2

1070 else: # y == 0

1071 r = PI if x < 0 else _0_0

1072 return Lam(Vermeille=r)

1073

1074 @Property_RO

1075 def latlon(self):

1076 '''Get the lat-, longitude in C{degrees} (L{LatLon2Tuple}C{(lat, lon)}).

1077 '''

1078 return LatLon2Tuple(self.lat, self.lon, name=self.name)

1079

1080 @Property_RO

1081 def latlonheight(self):

1082 '''Get the lat-, longitude in C{degrees} and height (L{LatLon3Tuple}C{(lat, lon, height)}).

1083 '''

1084 return self.latlon.to3Tuple(self.height)

1085

1086 @Property_RO

1087 def latlonheightdatum(self):

1088 '''Get the lat-, longitude in C{degrees} with height and datum (L{LatLon4Tuple}C{(lat, lon, height, datum)}).

1089 '''

1090 return self.latlonheight.to4Tuple(self.datum)

1091

1092 @Property_RO

1093 def latlonVermeille(self):

1094 '''Get the latitude and I{Vermeille} longitude in C{degrees [-225..+225]} (L{LatLon2Tuple}C{(lat, lon)}).

1095

1096 @see: Property C{lonVermeille}.

1097 '''

1098 return LatLon2Tuple(self.lat, self.lonVermeille, name=self.name)

1099

1100 @Property_RO

1101 def lonVermeille(self):

1102 '''Get the longitude in C{degrees [-225..+225]} after U{Vermeille

1103 <https://Search.ProQuest.com/docview/639493848>} (2004), p 95.

1104

1105 @see: Property C{lamVermeille}.

1106 '''

1107 return Lon(Vermeille=degrees(self.lamVermeille))

1108

1109 @Property_RO

1110 def phi(self):

1111 '''Get the latitude in C{radians} (C{float}).

1112 '''

1113 return self.philam.phi

1114

1115 @Property_RO

1116 def philam(self):

1117 '''Get the lat-, longitude in C{radians} (L{PhiLam2Tuple}C{(phi, lam)}).

1118 '''

1119 return PhiLam2Tuple(radians(self.lat), radians(self.lon), name=self.name)

1120

1121 @Property_RO

1122 def philamheight(self):

1123 '''Get the lat-, longitude in C{radians} and height (L{PhiLam3Tuple}C{(phi, lam, height)}).

1124 '''

1125 return self.philam.to3Tuple(self.height)

1126

1127 @Property_RO

1128 def philamheightdatum(self):

1129 '''Get the lat-, longitude in C{radians} with height and datum (L{PhiLam4Tuple}C{(phi, lam, height, datum)}).

1130 '''

1131 return self.philamheight.to4Tuple(self.datum)

1132

1133 @Property_RO

1134 def philamVermeille(self):

1135 '''Get the latitude and I{Vermeille} longitude in C{radians [-PI*3/2..+PI*3/2]} (L{PhiLam2Tuple}C{(phi, lam)}).

1136

1137 @see: Property C{lamVermeille}.

1138 '''

1139 return PhiLam2Tuple(radians(self.lat), self.lamVermeille, name=self.name)

1140

1141 def toCartesian(self, Cartesian=None, **Cartesian_kwds):

1142 '''Return the geocentric C{(x, y, z)} coordinates as an ellipsoidal or spherical

1143 C{Cartesian}.

1144

1145 @kwarg Cartesian: Optional class to return C{(x, y, z)} (L{ellipsoidalKarney.Cartesian},

1146 L{ellipsoidalNvector.Cartesian}, L{ellipsoidalVincenty.Cartesian},

1147 L{sphericalNvector.Cartesian} or L{sphericalTrigonometry.Cartesian})

1148 or C{None}.

1149 @kwarg Cartesian_kwds: Optional, additional B{C{Cartesian}} keyword arguments, ignored

1150 if C{B{Cartesian} is None}.

1151

1152 @return: A C{B{Cartesian}(x, y, z, **B{Cartesian_kwds})} instance or

1153 a L{Vector4Tuple}C{(x, y, z, h)} if C{B{Cartesian} is None}.

1154

1155 @raise TypeError: Invalid B{C{Cartesian}} or B{C{Cartesian_kwds}}.

1156 '''

1157 if Cartesian in (None, Vector4Tuple):

1158 r = self.xyzh

1159 elif Cartesian is Vector3Tuple:

1160 r = self.xyz

1161 else:

1162 _xsubclassof(self._CartesianBase, Cartesian=Cartesian)

1163 r = Cartesian(self, **_xkwds(Cartesian_kwds, name=self.name))

1164 return r

1165

1166 def toDatum(self, datum2):

1167 '''Convert this C{Ecef9Tuple} to an other datum.

1168

1169 @arg datum2: Datum to convert I{to} (L{Datum}).

1170

1171 @return: The converted 9-Tuple (C{Ecef9Tuple}).

1172

1173 @raise TypeError: The B{C{datum2}} is not a L{Datum}.

1174 '''

1175 if self.datum in (None, datum2): # PYCHOK _Names_

1176 r = self.copy()

1177 else:

1178 c = self._CartesianBase(self, datum=self.datum, name=self.name) # PYCHOK _Names_

1179 # c.toLatLon converts datum, x, y, z, lat, lon, etc.

1180 # and returns another Ecef9Tuple iff LatLon is None

1181 r = c.toLatLon(datum=datum2, LatLon=None)

1182 return r

1183

1184 def toLatLon(self, LatLon=None, **LatLon_kwds):

1185 '''Return the geodetic C{(lat, lon, height[, datum])} coordinates.

1186

1187 @kwarg LatLon: Optional class to return C{(lat, lon, height[, datum])}

1188 or C{None}.

1189 @kwarg LatLon_kwds: Optional B{C{height}}, B{C{datum}} and other

1190 B{C{LatLon}} keyword arguments.

1191

1192 @return: An instance of C{B{LatLon}(lat, lon, **B{LatLon_kwds})}

1193 or if B{C{LatLon}} is C{None}, a L{LatLon3Tuple}C{(lat, lon,

1194 height)} respectively L{LatLon4Tuple}C{(lat, lon, height,

1195 datum)} depending on whether C{datum} is un-/specified.

1196

1197 @raise TypeError: Invalid B{C{LatLon}} or B{C{LatLon_kwds}}.

1198 '''

1199 lat, lon, D = self.lat, self.lon, self.datum # PYCHOK Ecef9Tuple

1200 kwds = _xkwds(LatLon_kwds, height=self.height, datum=D, name=self.name) # PYCHOK Ecef9Tuple

1201 d = kwds.get(_datum_, LatLon)

1202 if LatLon is None:

1203 r = LatLon3Tuple(lat, lon, kwds[_height_], name=kwds[_name_])

1204 if d is not None:

1205 # assert d is not LatLon

1206 r = r.to4Tuple(d) # checks type(d)

1207 else:

1208 if d is None:

1209 _ = kwds.pop(_datum_) # remove None datum

1210 r = LatLon(lat, lon, **kwds)

1211 _xdatum(_xattr(r, datum=D), D)

1212 return r

1213

1214 def toLocal(self, ltp, Xyz=None, **Xyz_kwds):

1215 '''Convert this geocentric to I{local} C{x}, C{y} and C{z}.

1216

1217 @kwarg ltp: The I{local tangent plane} (LTP) to use (L{Ltp}).

1218 @kwarg Xyz: Optional class to return C{x}, C{y} and C{z}

1219 (L{XyzLocal}, L{Enu}, L{Ned}) or C{None}.

1220 @kwarg Xyz_kwds: Optional, additional B{C{Xyz}} keyword

1221 arguments, ignored if C{B{Xyz} is None}.

1222

1223 @return: An B{C{Xyz}} instance or if C{B{Xyz} is None},

1224 a L{Local9Tuple}C{(x, y, z, lat, lon, height,

1225 ltp, ecef, M)} with C{M=None}, always.

1226

1227 @raise TypeError: Invalid B{C{ltp}}.

1228 '''

1229 return _MODS.ltp._xLtp(ltp)._ecef2local(self, Xyz, Xyz_kwds)

1230

1231 def toVector(self, Vector=None, **Vector_kwds):

1232 '''Return the geocentric C{(x, y, z)} coordinates as vector.

1233

1234 @kwarg Vector: Optional vector class to return C{(x, y, z)} or

1235 C{None}.

1236 @kwarg Vector_kwds: Optional, additional B{C{Vector}} keyword

1237 arguments, ignored if C{B{Vector} is None}.

1238

1239 @return: A C{Vector}C{(x, y, z, **Vector_kwds)} instance or a

1240 L{Vector3Tuple}C{(x, y, z)} if B{C{Vector}} is C{None}.

1241

1242 @see: Propertes C{xyz} and C{xyzh}

1243 '''

1244 return self.xyz if Vector is None else Vector(

1245 *self.xyz, **_xkwds(Vector_kwds, name=self.name)) # PYCHOK Ecef9Tuple

1246

1247# def _T_x_M(self, T):

1248# '''(INTERNAL) Update M{self.M = T.multiply(self.M)}.

1249# '''

1250# return self.dup(M=T.multiply(self.M))

1251

1252 @Property_RO

1253 def xyz(self):

1254 '''Get the geocentric C{(x, y, z)} coordinates (L{Vector3Tuple}C{(x, y, z)}).

1255 '''

1256 return Vector3Tuple(self.x, self.y, self.z, name=self.name)

1257

1258 @Property_RO

1259 def xyzh(self):

1260 '''Get the geocentric C{(x, y, z)} coordinates and C{height} (L{Vector4Tuple}C{(x, y, z, h)})

1261 '''

1262 return self.xyz.to4Tuple(self.height)

1263

1264

1265 def _4Ecef(this, Ecef): # in .datums.Datum.ecef, .ellipsoids.Ellipsoid.ecef

1266 '''Return an ECEF converter for C{this} L{Datum} or L{Ellipsoid}.

1267 '''

1268 if Ecef is None:

1269 Ecef = EcefKarney

1270 else:

1271 _xinstanceof(*_Ecefs, Ecef=Ecef)

1272 return Ecef(this, name=this.name)

1273

1274

1275 def _llhn4(latlonh, lon, height, suffix=NN, Error=EcefError, name=NN): # in .ltp

1276 '''(INTERNAL) Get a C{(lat, lon, h, name)} 4-tuple.

1277 '''

1278 try:

1279 lat, lon = latlonh.lat, latlonh.lon

1280 h = _xattr(latlonh, height=_xattr(latlonh, h=height))

1281 n = _xattr(latlonh, name=NN)

1282 except AttributeError:

1283 lat, h, n = latlonh, height, NN

1284

1285 try:

1286 llhn = Lat(lat), Lon(lon), Height(h), (name or n)

1287 except (TypeError, ValueError) as x:

1288 t = _lat_, _lon_, _height_

1289 if suffix:

1290 t = (_ + suffix for _ in t)

1291 d = dict(zip(t, (lat, lon, h)))

1292 raise Error(cause=x, **d)

1293 return llhn

1294

1295

1296 def _xEcef(Ecef): # PYCHOK .latlonBase

1297 '''(INTERNAL) Validate B{C{Ecef}} I{class}.

1298 '''

1299 if issubclassof(Ecef, _EcefBase):

1300 return Ecef

1301 raise _TypesError(_Ecef_, Ecef, *_Ecefs)

1302

1303

1304# kwd lon00 unused but will throw a TypeError if misspelled, etc.

1305 def _xyzn4(xyz, y, z, Types, Error=EcefError, name=NN, # PYCHOK unused

1306 _xyz_y_z_names=_xyz_y_z, lon00=0): # in .ltp

1307 '''(INTERNAL) Get an C{(x, y, z, name)} 4-tuple.

1308 '''

1309 try:

1310 try:

1311 t = xyz.x, xyz.y, xyz.z, _xattr(xyz, name=name)

1312 if not isinstance(xyz, Types):

1313 raise _TypesError(_xyz_y_z_names[0], xyz, *Types)

1314 except AttributeError:

1315 t = map1(float, xyz, y, z) + (name,)

1316

1317 except (TypeError, ValueError) as x:

1318 d = dict(zip(_xyz_y_z_names, (xyz, y, z)))

1319 raise Error(cause=x, **d)

1320 return t

1321# assert _xyz_y_z == _MODS.basics._xargs_kwds_names(_xyzn4)[:3]

1322

1323

1324_Ecefs = (EcefKarney, EcefSudano, EcefVeness, EcefYou,

1325 EcefFarrell21, EcefFarrell22)

1326__all__ += _ALL_DOCS(_EcefBase)

1327

1328# **) MIT License

1329#

1330# Copyright (C) 2016-2024 -- mrJean1 at Gmail -- All Rights Reserved.

1331#

1332# Permission is hereby granted, free of charge, to any person obtaining a

1333# copy of this software and associated documentation files (the "Software"),

1334# to deal in the Software without restriction, including without limitation

1335# the rights to use, copy, modify, merge, publish, distribute, sublicense,

1336# and/or sell copies of the Software, and to permit persons to whom the

1337# Software is furnished to do so, subject to the following conditions:

1338#

1339# The above copyright notice and this permission notice shall be included

1340# in all copies or substantial portions of the Software.

1341#

1342# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

1343# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

1344# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

1345# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

1346# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

1347# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

1348# OTHER DEALINGS IN THE SOFTWARE.