1

2# -*- coding: utf-8 -*-

3

4 u'''Ellipsoidal, C{N-vector}-based geodesy.

5

6 Ellipsoidal classes geodetic (lat-/longitude) L{LatLon}, geocentric

7(ECEF) L{Cartesian}, DEPRECATED L{Ned} and L{Nvector} and functions

8 L{meanOf}, L{sumOf} and DEPRECATED L{toNed}.

9

10 Pure Python implementation of n-vector-based geodetic (lat-/longitude)

11 methods by I{(C) Chris Veness 2011-2016} published under the same MIT

12 Licence**, see U{Vector-based geodesy

13<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}.

14

15 These classes and functions work with: (a) geodesic (polar) lat-/longitude

16 points on the earth's surface and (b) 3-D vectors used as n-vectors

17 representing points on the earth's surface or vectors normal to the plane

18 of a great circle.

19

20 See also Kenneth Gade U{'A Non-singular Horizontal Position Representation'

21<https://www.NavLab.net/Publications/A_Nonsingular_Horizontal_Position_Representation.pdf>},

22 The Journal of Navigation (2010), vol 63, nr 3, pp 395-417.

23'''

24# make sure int/int division yields float quotient, see .basics

25 from __future__ import division as _; del _ # PYCHOK semicolon

26

27 from pygeodesy.basics import issubclassof, map2, _xinstanceof

28 from pygeodesy.datums import _ellipsoidal_datum, _spherical_datum, _WGS84

29# from pygeodesy.dms import toDMS # _MODS

30 from pygeodesy.ellipsoidalBase import CartesianEllipsoidalBase, intersecant2, \

31 _nearestOn, LatLonEllipsoidalBase, \

32 _TOL_M, _Wrap

33 from pygeodesy.errors import _IsnotError, _xkwds

34# from pygeodesy.fmath import fdot # from .nvectorBase

35 from pygeodesy.interns import NN, _Nv00_, _COMMASPACE_

36 from pygeodesy.interns import _down_, _east_, _north_, _pole_ # PYCHOK used!

37 from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS, _ALL_OTHER

38# from pygeodesy.ltp import Ltp # _MODS

39 from pygeodesy.ltpTuples import Aer as _Aer, Ned as _Ned, Ned4Tuple, \

40 sincos2d_, _xnamed

41# from pygeodesy.named import _xnamed # from .ltpTuples

42 from pygeodesy.nvectorBase import fabs, fdot, NorthPole, LatLonNvectorBase, \

43 NvectorBase, sumOf as _sumOf

44 from pygeodesy.props import deprecated_class, deprecated_function, \

45 deprecated_method, Property_RO

46 from pygeodesy.streprs import Fmt, fstr, _xzipairs

47 from pygeodesy.units import Bearing, Distance, Height, Scalar

48# from pygeodesy.utily import sincos2d_, _Wrap # from .ltpTuples, .ellipsoidalBase

49

50# from math import fabs # from .nvectorBase

51

52__all__ = _ALL_LAZY.ellipsoidalNvector

53__version__ = '23.10.08'

54

55

56 class Ned(_Ned):

57 '''DEPRECATED, use class L{pygeodesy.Ned}.'''

58

59 def __init__(self, north, east, down, name=NN):

60 deprecated_class(self.__class__)

61 _Ned.__init__(self, north, east, down, name=name)

62

63 @deprecated_method # PYCHOK expected

64 def toRepr(self, prec=None, fmt=Fmt.SQUARE, sep=_COMMASPACE_, **unused):

65 '''DEPRECATED, use class L{pygeodesy.Ned}.

66

67 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

68 @kwarg fmt: Enclosing backets format (C{str}).

69 @kwarg sep: Separator between NEDs (C{str}).

70

71 @return: This Ned as "[L:f, B:degrees360, E:degrees90]" (C{str})

72 with length or slantrange C{L}, bearing or azimuth C{B}

73 and elevation C{E}.

74 '''

75 dms = _MODS.dms

76 t = (fstr(self.slantrange, prec=3 if prec is None else prec),

77 dms.toDMS(self.azimuth, form=dms.F_D, prec=prec, ddd=0),

78 dms.toDMS(self.elevation, form=dms.F_D, prec=prec, ddd=0))

79 return _xzipairs('LBE', t, sep=sep, fmt=fmt)

80

81

82 class Cartesian(CartesianEllipsoidalBase):

83 '''Extended to convert geocentric, L{Cartesian} points to

84 L{Nvector} and n-vector-based, geodetic L{LatLon}.

85 '''

86 @Property_RO

87 def Ecef(self):

88 '''Get the ECEF I{class} (L{EcefVeness}), I{lazily}.

89 '''

90 return _MODS.ecef.EcefVeness

91

92 def toLatLon(self, **LatLon_and_kwds): # PYCHOK LatLon=LatLon, datum=None

93 '''Convert this cartesian to an C{Nvector}-based geodetic point.

94

95 @kwarg LatLon_and_kwds: Optional L{LatLon}, B{C{datum}} and other

96 keyword arguments. Use C{B{LatLon}=...} to

97 override this L{LatLon} class or specify

98 C{B{LatLon} is None}.

99

100 @return: The geodetic point (L{LatLon}) or if B{C{LatLon}} is set

101 to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height,

102 C, M, datum)} with C{C} and C{M} if available.

103

104 @raise TypeError: Invalid B{C{LatLon_and_kwds}}.

105 '''

106 kwds = _xkwds(LatLon_and_kwds, LatLon=LatLon, datum=self.datum)

107 return CartesianEllipsoidalBase.toLatLon(self, **kwds)

108

109 def toNvector(self, **Nvector_and_kwds): # PYCHOK Datums.WGS84

110 '''Convert this cartesian to L{Nvector} components, I{including height}.

111

112 @kwarg Nvector_and_kwds: Optional L{Nvector}, B{C{datum}} and other

113 keyword arguments. Use C{B{Nvector}=...} to

114 override this L{Nvector} class or specify

115 C{B{Nvector} is None}.

116

117 @return: The C{n-vector} components (L{Nvector}) or if B{C{Nvector}}

118 is set to C{None}, a L{Vector4Tuple}C{(x, y, z, h)}

119

120 @raise TypeError: Invalid B{C{Nvector_and_kwds}}.

121

122 @example:

123

124 >>> from ellipsoidalNvector import LatLon

125 >>> c = Cartesian(3980581, 97, 4966825)

126 >>> n = c.toNvector() # (0.62282, 0.000002, 0.78237, +0.24)

127 '''

128 kwds = _xkwds(Nvector_and_kwds, Nvector=Nvector, datum=self.datum)

129 return CartesianEllipsoidalBase.toNvector(self, **kwds)

130

131

132 class LatLon(LatLonNvectorBase, LatLonEllipsoidalBase):

133 '''An n-vector-based, ellipsoidal L{LatLon} point.

134

135 @example:

136

137 >>> from ellipsoidalNvector import LatLon

138 >>> p = LatLon(52.205, 0.119) # height=0, datum=Datums.WGS84

139 '''

140 _Nv = None # cached toNvector (L{Nvector})

141

142 def _update(self, updated, *attrs, **setters): # PYCHOK args

143 '''(INTERNAL) Zap cached attributes if updated.

144 '''

145 if updated:

146 LatLonNvectorBase._update(self, updated, _Nv=self._Nv) # special case

147 LatLonEllipsoidalBase._update(self, updated, *attrs, **setters)

148

149# def crossTrackDistanceTo(self, start, end, radius=R_M):

150# '''Return the (signed) distance from this point to the great

151# circle defined by a start point and an end point or bearing.

152#

153# @arg start: Start point of great circle line (L{LatLon}).

154# @arg end: End point of great circle line (L{LatLon}) or

155# initial bearing (compass C{degrees360}) at the

156# start point.

157# @kwarg radius: Mean earth radius (C{meter}).

158#

159# @return: Distance to great circle, negative if to left or

160# positive if to right of line (C{meter}, same units

161# as B{C{radius}}).

162#

163# @raise TypeError: If B{C{start}} or B{C{end}} point is not L{LatLon}.

164#

165# @example:

166#

167# >>> p = LatLon(53.2611, -0.7972)

168#

169# >>> s = LatLon(53.3206, -1.7297)

170# >>> b = 96.0

171# >>> d = p.crossTrackDistanceTo(s, b) # -305.7

172#

173# >>> e = LatLon(53.1887, 0.1334)

174# >>> d = p.crossTrackDistanceTo(s, e) # -307.5

175# '''

176# self.others(start=start)

177#

178# if isscalar(end): # gc from point and bearing

179# gc = start.greatCircle(end)

180# else: # gc by two points

181# gc = start.toNvector().cross(end.toNvector())

182#

183# # (signed) angle between point and gc normal vector

184# v = self.toNvector()

185# a = gc.angleTo(v, vSign=v.cross(gc))

186# a = _copysign(PI_2, a) - a

187# return a * float(radius)

188

189 def deltaTo(self, other, Ned=Ned, wrap=False):

190 '''Calculate the local delta from this to an other point.

191

192 @note: This is a linear delta, I{unrelated} to a geodesic

193 on the ellipsoid.

194

195 @arg other: The other point (L{LatLon}).

196 @kwarg Ned: Class to use (L{pygeodesy.Ned} or

197 L{pygeodesy.Ned4Tuple}), overriding the

198 default DEPRECATED L{Ned}.

199 @kwarg wrap: If C{True}, wrap or I{normalize} the

200 B{C{other}} point (C{bool}).

201

202 @return: Delta from this to the other point (B{C{Ned}}).

203

204 @raise TypeError: The B{C{other}} point is not L{LatLon} or

205 B{C{Ned}} is not L{pygeodesy.Ned} nor

206 L{pygeodesy.Ned4Tuple} nor DEPRECATED L{Ned}.

207

208 @raise ValueError: If ellipsoids are incompatible.

209

210 @example:

211

212 >>> a = LatLon(49.66618, 3.45063)

213 >>> b = LatLon(48.88667, 2.37472)

214 >>> delta = a.deltaTo(b) # [N:-86126, E:-78900, D:1069]

215 >>> d = delta.length # 116807.681 m

216 >>> b = delta.bearing # 222.493°

217 >>> e = delta.elevation # -0.5245°

218 '''

219 self.ellipsoids(other) # throws TypeError and ValueError

220

221 p = self.others(other)

222 if wrap:

223 p = _Wrap.point(p)

224 # get delta in cartesian frame

225 dc = p.toCartesian().minus(self.toCartesian())

226 # rotate dc to get delta in n-vector reference

227 # frame using the rotation matrix row vectors

228 ned_ = map2(dc.dot, self._rotation3)

229 if issubclassof(Ned, Ned4Tuple):

230 ned_ += (_MODS.ltp.Ltp(self, ecef=self.Ecef(self.datum)),)

231 elif not issubclassof(Ned, _Ned):

232 raise _IsnotError(Fmt.sub_class(_Ned, Ned4Tuple), Ned=Ned)

233 return Ned(*ned_, name=self.name)

234

235# def destination(self, distance, bearing, radius=R_M, height=None):

236# '''Return the destination point after traveling from this

237# point the given distance on the given initial bearing.

238#

239# @arg distance: Distance traveled (C{meter}, same units as

240# given earth B{C{radius}}).

241# @arg bearing: Initial bearing (compass C{degrees360}).

242# @kwarg radius: Mean earth radius (C{meter}).

243# @kwarg height: Optional height at destination point,

244# overriding default (C{meter}, same units

245# as B{C{radius}}).

246#

247# @return: Destination point (L{LatLon}).

248#

249# @example:

250#

251# >>> p = LatLon(51.4778, -0.0015)

252# >>> q = p.destination(7794, 300.7)

253# >>> q.toStr() # '51.5135°N, 000.0983°W' ?

254# '''

255# r = _angular(distance, radius) # angular distance in radians

256# # great circle by starting from this point on given bearing

257# gc = self.greatCircle(bearing)

258#

259# v1 = self.toNvector()

260# x = v1.times(cos(r)) # component of v2 parallel to v1

261# y = gc.cross(v1).times(sin(r)) # component of v2 perpendicular to v1

262#

263# v2 = x.plus(y).unit()

264# return v2.toLatLon(height=self.height if height is C{None} else height)

265

266 def destinationNed(self, delta):

267 '''Calculate the destination point using the supplied NED delta

268 from this point.

269

270 @arg delta: Delta from this to the other point in the local

271 tangent plane (LTP) of this point (L{Ned}).

272

273 @return: Destination point (L{LatLon}).

274

275 @raise TypeError: If B{C{delta}} is not L{pygeodesy.Ned} or

276 DEPRECATED L{Ned}.

277

278 @example:

279

280 >>> a = LatLon(49.66618, 3.45063)

281 >>> delta = Ned(-86126, -78900, 1069) # from Aer(222.493, -0.5245, 116807.681)

282 >>> b = a.destinationNed(delta) # 48.886669°N, 002.374721°E or 48°53′12.01″N, 002°22′29.0″E +0.20m

283 '''

284 _xinstanceof(_Ned, delta=delta)

285

286 nv, ev, dv = self._rotation3

287 # convert NED delta to standard coordinate frame of n-vector

288 dn = delta.ned

289 # rotate dn to get delta in cartesian (ECEF) coordinate

290 # reference frame using the rotation matrix column vectors

291 dc = Cartesian(fdot(dn, nv.x, ev.x, dv.x),

292 fdot(dn, nv.y, ev.y, dv.y),

293 fdot(dn, nv.z, ev.z, dv.z))

294

295 # apply (cartesian) delta to this Cartesian to obtain destination as cartesian

296 v = self.toCartesian().plus(dc)

297 return v.toLatLon(datum=self.datum, LatLon=self.classof) # Cartesian(v.x, v.y, v.z).toLatLon(...)

298

299 def distanceTo(self, other, radius=None, wrap=False):

300 '''I{Approximate} the distance from this to an other point.

301

302 @arg other: The other point (L{LatLon}).

303 @kwarg radius: Mean earth radius, ellipsoid or datum (C{meter},

304 L{Ellipsoid}, L{Ellipsoid2}, L{Datum} or

305 L{a_f2Tuple}), overriding the mean radius C{R1}

306 of this point's datum..

307 @kwarg wrap: If C{True}, wrap or I{normalize} and unroll the

308 B{C{other}} and angular distance (C{bool}).

309

310 @return: Distance (C{meter}, same units as B{C{radius}}).

311

312 @raise TypeError: The B{C{other}} point is not L{LatLon}.

313

314 @raise ValueError: Invalid B{C{radius}}.

315

316 @example:

317

318 >>> p = LatLon(52.205, 0.119)

319 >>> q = LatLon(48.857, 2.351);

320 >>> d = p.distanceTo(q) # 404300

321 '''

322 p = self.others(other)

323 if wrap:

324 p = _Wrap.point(p)

325 a = self._N_vector.angleTo(p._N_vector, wrap=wrap)

326 d = self.datum if radius is None else _spherical_datum(radius)

327 return fabs(a) * d.ellipsoid.R1 # see .utily.radians2m

328

329 @Property_RO

330 def Ecef(self):

331 '''Get the ECEF I{class} (L{EcefVeness}), I{lazily}.

332 '''

333 return _MODS.ecef.EcefVeness

334

335 @deprecated_method

336 def equals(self, other, eps=None): # PYCHOK no cover

337 '''DEPRECATED, use method L{isequalTo}.

338 '''

339 return self.isequalTo(other, eps=eps)

340

341 def isequalTo(self, other, eps=None):

342 '''Compare this point with an other point.

343

344 @arg other: The other point (L{LatLon}).

345 @kwarg eps: Optional margin (C{float}).

346

347 @return: C{True} if points are identical, including

348 datum, I{ignoring height}, C{False} otherwise.

349

350 @raise TypeError: The B{C{other}} point is not L{LatLon}.

351

352 @raise ValueError: Invalid B{C{eps}}.

353

354 @see: Method C{isequalTo3} to include I{height}.

355

356 @example:

357

358 >>> p = LatLon(52.205, 0.119)

359 >>> q = LatLon(52.205, 0.119)

360 >>> e = p.isequalTo(q) # True

361 '''

362 return self.datum == self.others(other).datum and \

363 _MODS.formy._isequalTo(self, other, eps=eps)

364

365# def greatCircle(self, bearing):

366# '''Return the great circle heading on the given bearing

367# from this point.

368#

369# Direction of vector is such that initial bearing vector

370# b = c × p, where p is representing this point.

371#

372# @arg bearing: Bearing from this point (compass C{degrees360}).

373#

374# @return: N-vector representing great circle (L{Nvector}).

375#

376# @example:

377#

378# >>> p = LatLon(53.3206, -1.7297)

379# >>> g = p.greatCircle(96.0)

380# >>> g.toStr() # '(-0.794, 0.129, 0.594)'

381# '''

382# a, b, _ = self.philamheight

383# t = radians(bearing)

384#

385# sa, ca, sb, cb, st, ct = sincos2_(a, b, t)

386# return self._xnamed(Nvector(sb * ct - sa * cb * st,

387# -cb * ct - sa * sb * st,

388# ca * st)

389

390# def initialBearingTo(self, other, wrap=False):

391# '''Return the initial bearing (forward azimuth) from

392# this to an other point.

393#

394# @arg other: The other point (L{LatLon}).

395# @kwarg wrap: If C{True}, wrap or I{normalize}

396# and unroll the B{C{other}} (C{bool}).

397#

398# @return: Initial bearing (compass C{degrees360}).

399#

400# @raise TypeError: The B{C{other}} point is not L{LatLon}.

401#

402# @example:

403#

404# >>> p1 = LatLon(52.205, 0.119)

405# >>> p2 = LatLon(48.857, 2.351)

406# >>> b = p1.bearingTo(p2) # 156.2

407# '''

408# p = self.others(other)

409# if wrap:

410# p = _Wrap.point(p)

411# v1 = self.toNvector()

412#

413# gc1 = v1.cross(p.toNvector()) # gc through v1 & v2

414# gc2 = v1.cross(_NP3) # gc through v1 & North pole

415#

416# # bearing is (signed) angle between gc1 & gc2

417# return degrees360(gc1.angleTo(gc2, vSign=v1))

418

419 def intermediateTo(self, other, fraction, height=None, wrap=False):

420 '''Return the point at given fraction between this and

421 an other point.

422

423 @arg other: The other point (L{LatLon}).

424 @arg fraction: Fraction between both points (C{scalar},

425 0.0 at this to 1.0 at the other point.

426 @kwarg height: Optional height, overriding the fractional

427 height (C{meter}).

428 @kwarg wrap: If C{True}, wrap or I{normalize} the

429 B{C{other}} point (C{bool}).

430

431 @return: Intermediate point (L{LatLon}).

432

433 @raise TypeError: The B{C{other}} point is not L{LatLon}.

434

435 @example:

436

437 >>> p = LatLon(52.205, 0.119)

438 >>> q = LatLon(48.857, 2.351)

439 >>> p = p.intermediateTo(q, 0.25) # 51.3721°N, 000.7073°E

440 '''

441 p = self.others(other)

442 if wrap:

443 p = _Wrap.point(p)

444 f = Scalar(fraction=fraction)

445 h = self._havg(other, f=f, h=height)

446 i = self.toNvector().intermediateTo(p.toNvector(), f)

447 return i.toLatLon(height=h, LatLon=self.classof) # Nvector(i.x, i.y, i.z).toLatLon(...)

448

449 @Property_RO

450 def _rotation3(self):

451 '''(INTERNAL) Get the rotation matrix from n-vector coordinate frame axes.

452 '''

453 nv = self.toNvector() # local (n-vector) coordinate frame

454

455 dv = nv.negate() # down, opposite to n-vector

456 ev = NorthPole.cross(nv, raiser=_pole_).unit() # east, pointing perpendicular to the plane

457 nv = ev.cross(dv) # north, by right hand rule

458 return nv, ev, dv # matrix rows

459

460 def toCartesian(self, **Cartesian_and_kwds): # PYCHOK Cartesian=Cartesian, datum=None

461 '''Convert this point to an C{Nvector}-based geodetic point.

462

463 @kwarg Cartesian_and_kwds: Optional L{Cartesian}, B{C{datum}} and other

464 keyword arguments. Use C{B{Cartesian}=...}

465 to override this L{Cartesian} class or specify

466 C{B{Cartesian}=None}.

467

468 @return: The geodetic point (L{Cartesian}) or if B{C{Cartesian}} is set

469 to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M,

470 datum)} with C{C} and C{M} if available.

471

472 @raise TypeError: Invalid B{C{Cartesian}} or other B{C{Cartesian_and_kwds}}.

473 '''

474 kwds = _xkwds(Cartesian_and_kwds, Cartesian=Cartesian, datum=self.datum)

475 return LatLonEllipsoidalBase.toCartesian(self, **kwds)

476

477 def toNvector(self, **Nvector_and_kwds): # PYCHOK signature

478 '''Convert this point to L{Nvector} components, I{including height}.

479

480 @kwarg Nvector_and_kwds: Optional L{Nvector}, B{C{datum}} and other

481 keyword arguments. Use C{B{Nvector}=...}

482 to override this L{Nvector} class or specify

483 C{B{Nvector}=None}.

484

485 @return: The C{n-vector} components (L{Nvector}) or if B{C{Nvector}}

486 is set to C{None}, a L{Vector4Tuple}C{(x, y, z, h)}.

487

488 @raise TypeError: Invalid B{C{Nvector}} or other B{C{Nvector_and_kwds}}.

489

490 @example:

491

492 >>> p = LatLon(45, 45)

493 >>> n = p.toNvector()

494 >>> n.toStr() # [0.50, 0.50, 0.70710]

495 '''

496 kwds = _xkwds(Nvector_and_kwds, Nvector=Nvector, datum=self.datum)

497 return LatLonNvectorBase.toNvector(self, **kwds)

498

499

500_Nvll = LatLon(0, 0, name=_Nv00_) # reference instance (L{LatLon})

501

502

503 class Nvector(NvectorBase):

504 '''An n-vector is a position representation using a (unit) vector

505 normal to the earth ellipsoid. Unlike lat-/longitude points,

506 n-vectors have no singularities or discontinuities.

507

508 For many applications, n-vectors are more convenient to work

509 with than other position representations like lat-/longitude,

510 earth-centred earth-fixed (ECEF) vectors, UTM coordinates, etc.

511

512 Note commonality with L{sphericalNvector.Nvector}.

513 '''

514 _datum = _WGS84 # default datum (L{Datum})

515

516 def __init__(self, x_xyz, y=None, z=None, h=0, datum=None, ll=None, name=NN):

517 '''New n-vector normal to the earth's surface.

518

519 @arg x_xyz: X component of vector (C{scalar}) or (3-D) vector

520 (C{Nvector}, L{Vector3d}, L{Vector3Tuple} or

521 L{Vector4Tuple}).

522 @kwarg y: Y component of vector (C{scalar}), ignored if B{C{x_xyz}}

523 is not C{scalar}, otherwise same units as B{C{x_xyz}}.

524 @kwarg z: Z component of vector (C{scalar}), ignored if B{C{x_xyz}}

525 is not C{scalar}, otherwise same units as B{C{x_xyz}}.

526 @kwarg h: Optional height above model surface (C{meter}).

527 @kwarg datum: Optional datum this n-vector is defined in

528 (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or

529 L{a_f2Tuple}).

530 @kwarg ll: Optional, original latlon (C{LatLon}).

531 @kwarg name: Optional name (C{str}).

532

533 @raise TypeError: If B{C{datum}} is not a L{Datum}.

534

535 @example:

536

537 >>> from ellipsoidalNvector import Nvector

538 >>> v = Nvector(0.5, 0.5, 0.7071, 1)

539 >>> v.toLatLon() # 45.0°N, 045.0°E, +1.00m

540 '''

541 NvectorBase.__init__(self, x_xyz, y=y, z=z, h=h, ll=ll, name=name)

542 if datum not in (None, self._datum):

543 self._datum = _ellipsoidal_datum(datum, name=name)

544

545 @Property_RO

546 def datum(self):

547 '''Get this n-vector's datum (L{Datum}).

548 '''

549 return self._datum

550

551 def toCartesian(self, **Cartesian_and_kwds): # PYCHOK Cartesian=Cartesian

552 '''Convert this n-vector to C{Nvector}-based cartesian (ECEF) coordinates.

553

554 @kwarg Cartesian_and_kwds: Optional L{Cartesian}, B{C{h}}, B{C{datum}} and

555 other keyword arguments. Use C{B{Cartesian}=...}

556 to override this L{Cartesian} class or specify

557 C{B{Cartesian} is None}.

558

559 @return: The cartesian point (L{Cartesian}) or if B{C{Cartesian}} is set

560 to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M,

561 datum)} with C{C} and C{M} if available.

562

563 @raise TypeError: Invalid B{C{Cartesian_and_kwds}}.

564

565 @example:

566

567 >>> v = Nvector(0.5, 0.5, 0.7071)

568 >>> c = v.toCartesian() # [3194434, 3194434, 4487327]

569 >>> p = c.toLatLon() # 45.0°N, 45.0°E

570 '''

571 kwds = _xkwds(Cartesian_and_kwds, h=self.h, Cartesian=Cartesian,

572 datum=self.datum)

573 return NvectorBase.toCartesian(self, **kwds) # class or .classof

574

575 def toLatLon(self, **LatLon_and_kwds): # PYCHOK height=None, LatLon=LatLon

576 '''Convert this n-vector to an C{Nvector}-based geodetic point.

577

578 @kwarg LatLon_and_kwds: Optional L{LatLon}, B{C{height}}, B{C{datum}}

579 and other keyword arguments. Use C{B{LatLon}=...}

580 to override this L{LatLon} class or specify

581 C{B{LatLon} is None}.

582

583 @return: The geodetic point (L{LatLon}) or if B{C{LatLon}} is set

584 to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height,

585 C, M, datum)} with C{C} and C{M} if available.

586

587 @raise TypeError: Invalid B{C{LatLon_and_kwds}}.

588

589 @example:

590

591 >>> v = Nvector(0.5, 0.5, 0.7071)

592 >>> p = v.toLatLon() # 45.0°N, 45.0°E

593 '''

594 kwds = _xkwds(LatLon_and_kwds, height=self.h, datum=self.datum, LatLon=LatLon)

595 return NvectorBase.toLatLon(self, **kwds) # class or .classof

596

597 def unit(self, ll=None):

598 '''Normalize this vector to unit length.

599

600 @kwarg ll: Optional, original latlon (C{LatLon}).

601

602 @return: Normalised vector (L{Nvector}).

603 '''

604 u = NvectorBase.unit(self, ll=ll)

605 if u.datum != self.datum:

606 u._update(False, datum=self.datum)

607 return u

608

609

610 def meanOf(points, datum=_WGS84, height=None, wrap=False,

611 **LatLon_and_kwds):

612 '''Compute the geographic mean of several points.

613

614 @arg points: Points to be averaged (L{LatLon}[]).

615 @kwarg datum: Optional datum to use (L{Datum}).

616 @kwarg height: Optional height at mean point, overriding

617 the mean height (C{meter}).

618 @kwarg wrap: If C{True}, wrap or I{normalize} B{C{points}}

619 (C{bool}).

620 @kwarg LatLon_and_kwds: Optional B{C{LatLon}} class to return

621 the mean points and overriding this L{LatLon}

622 (or C{None}) and additional B{C{LatLon}}

623 keyword arguments, ignored if C{B{LatLon}

624 is None}.

625

626 @return: Geographic mean point and mean height (B{C{LatLon}})

627 or if B{C{LatLon}} is C{None}, an L{Ecef9Tuple}C{(x,

628 y, z, lat, lon, height, C, M, datum)} with C{C} and

629 C{M} if available.

630

631 @raise ValueError: Insufficient number of B{C{points}}.

632 '''

633 Ps = _Nvll.PointsIter(points, wrap=wrap)

634 # geographic mean

635 m = sumOf(p._N_vector for p in Ps.iterate(closed=False))

636 kwds = _xkwds(LatLon_and_kwds, height=height, datum=datum,

637 LatLon=LatLon, name=meanOf.__name__)

638 return m.toLatLon(**kwds)

639

640

641 def nearestOn(point, point1, point2, within=True, height=None, wrap=False,

642 equidistant=None, tol=_TOL_M, LatLon=LatLon, **LatLon_kwds):

643 '''I{Iteratively} locate the closest point on the geodesic between

644 two other (ellipsoidal) points.

645

646 @arg point: Reference point (C{LatLon}).

647 @arg point1: Start point of the geodesic (C{LatLon}).

648 @arg point2: End point of the geodesic (C{LatLon}).

649 @kwarg within: If C{True} return the closest point I{between}

650 B{C{point1}} and B{C{point2}}, otherwise the

651 closest point elsewhere on the geodesic (C{bool}).

652 @kwarg height: Optional height for the closest point (C{meter},

653 conventionally) or C{None} or C{False} for the

654 interpolated height. If C{False}, the closest

655 takes the heights of the points into account.

656 @kwarg wrap: If C{True}, wrap or I{normalize} and unroll I{only}

657 B{C{point1}} and B{C{point2}} (C{bool}).

658 @kwarg equidistant: An azimuthal equidistant projection (I{class}

659 or function L{pygeodesy.equidistant}) or C{None}

660 for the preferred C{B{point}.Equidistant}.

661 @kwarg tol: Convergence tolerance (C{meter}).

662 @kwarg LatLon: Optional class to return the closest point

663 (L{LatLon}) or C{None}.

664 @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword

665 arguments, ignored if C{B{LatLon} is None}.

666

667 @return: Closest point, a B{C{LatLon}} instance or if C{B{LatLon}

668 is None}, a L{LatLon4Tuple}C{(lat, lon, height, datum)}.

669

670 @raise ImportError: Package U{geographiclib

671 <https://PyPI.org/project/geographiclib>}

672 not installed or not found.

673

674 @raise TypeError: Invalid or non-ellipsoidal B{C{point}}, B{C{point1}}

675 or B{C{point2}} or invalid B{C{equidistant}}.

676

677 @raise ValueError: No convergence for the B{C{tol}}.

678

679 @see: U{The B{ellipsoidal} case<https://GIS.StackExchange.com/questions/48937/

680 calculating-intersection-of-two-circles>} and U{Karney's paper

681 <https://ArXiv.org/pdf/1102.1215.pdf>}, pp 20-21, section B{14. MARITIME

682 BOUNDARIES} for more details about the iteration algorithm.

683 '''

684 return _nearestOn(point, point1, point2, within=within, height=height, wrap=wrap,

685 equidistant=equidistant, tol=tol, LatLon=LatLon, **LatLon_kwds)

686

687

688 def sumOf(nvectors, Vector=Nvector, h=None, **Vector_kwds):

689 '''Return the vectorial sum of two or more n-vectors.

690

691 @arg nvectors: Vectors to be added (L{Nvector}[]).

692 @kwarg Vector: Optional class for the vectorial sum (L{Nvector}).

693 @kwarg h: Optional height, overriding the mean height (C{meter}).

694 @kwarg Vector_kwds: Optional, additional B{C{Vector}} keyword

695 arguments, ignored if C{B{Vector} is None}.

696

697 @return: Vectorial sum (B{C{Vector}}).

698

699 @raise VectorError: No B{C{nvectors}}.

700 '''

701 return _sumOf(nvectors, Vector=Vector, h=h, **Vector_kwds)

702

703

704@deprecated_function

705 def toNed(distance, bearing, elevation, Ned=Ned, name=NN):

706 '''DEPRECATED, use L{pygeodesy.Aer}C{(bearing, elevation,

707 distance).xyzLocal.toNed(B{Ned}, name=B{name})} or

708 L{XyzLocal}C{(pygeodesy.Aer(bearing, elevation,

709 distance)).toNed(B{Ned}, name=B{name})}.

710

711 Create an NED vector from distance, bearing and elevation

712 (in local coordinate system).

713

714 @arg distance: NED vector length (C{meter}).

715 @arg bearing: NED vector bearing (compass C{degrees360}).

716 @arg elevation: NED vector elevation from local coordinate

717 frame horizontal (C{degrees}).

718 @kwarg Ned: Optional class to return the NED (C{Ned}) or

719 C{None}.

720 @kwarg name: Optional name (C{str}).

721

722 @return: An NED vector equivalent to this B{C{distance}},

723 B{C{bearing}} and B{C{elevation}} (DEPRECATED L{Ned})

724 or a DEPRECATED L{Ned3Tuple}C{(north, east, down)}

725 if C{B{Ned} is None}.

726

727 @raise ValueError: Invalid B{C{distance}}, B{C{bearing}}

728 or B{C{elevation}}.

729 '''

730 if True: # use new Aer class

731 n, e, d, _ = _Aer(bearing, elevation, distance).xyz4

732 else: # DEPRECATED

733 d = Distance(distance)

734

735 sb, cb, se, ce = sincos2d_(Bearing(bearing),

736 Height(elevation=elevation))

737 n = cb * d * ce

738 e = sb * d * ce

739 d *= se

740

741 r = _MODS.deprecated.Ned3Tuple(n, e, -d) if Ned is None else \

742 Ned(n, e, -d)

743 return _xnamed(r, name)

744

745

746__all__ += _ALL_OTHER(Cartesian, LatLon, Ned, Nvector, # classes

747 intersecant2, # from .ellipsoidalBase

748 meanOf, sumOf, toNed)

749

750# **) MIT License

751#

752# Copyright (C) 2016-2023 -- mrJean1 at Gmail -- All Rights Reserved.

753#

754# Permission is hereby granted, free of charge, to any person obtaining a

755# copy of this software and associated documentation files (the "Software"),

756# to deal in the Software without restriction, including without limitation

757# the rights to use, copy, modify, merge, publish, distribute, sublicense,

758# and/or sell copies of the Software, and to permit persons to whom the

759# Software is furnished to do so, subject to the following conditions:

760#

761# The above copyright notice and this permission notice shall be included

762# in all copies or substantial portions of the Software.

763#

764# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

765# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

766# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

767# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

768# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

769# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

770# OTHER DEALINGS IN THE SOFTWARE.