# spacepy.irbempy.coord_trans

spacepy.irbempy.coord_trans(loci, returntype, returncarsph)

  thin layer to call coor_trans1 from irbem lib this will convert between systems GDZ, GEO, GSM, GSE, SM, GEI, MAG, SPH, RLL

  Parameters:
    - loci (Coords instance)containing coordinate information, can contain n points
    - returntype (str)describing system as GDZ, GEO, GSM, GSE, SM, GEI, MAG, SPH, RLL
    - returncarsph (str)cartesian or spherical units ‘car’, ‘sph’
  Returns:
    - xout (ndarray)values after transformation in (n,3) dimensions

  See also

  `sph2car`, `car2sph`

  Examples

      >>> c = Coords([[3,0,0],[2,0,0]], 'GEO', 'car', use_irbem=True)
      >>> c.ticks = Ticktock(['2002-02-02T12:00:00', '2002-02-02T12:10:00'], 'ISO')
      >>> coord_trans(c, 'GSM', 'car')
      array([[ 2.8639301 , -0.01848784,  0.89306361],
      [ 1.9124434 ,  0.07209424,  0.58082929]])