Measurement performed the 19th February 2018 on an Anritsu MS46524B 20GHz Vector Network Analyser.
The setup is a linear frequency sweep from 1MHz to 10GHz with 1MHz step, 10'000 points.
If bandwidth 1kHz, 0dBm output power, no smoothing, no averaging.
