Package pygeodesy :: Module ellipsoidalBaseDI :: Class LatLonEllipsoidalBaseDI |
[frames] | no frames]

# Class LatLonEllipsoidalBaseDI

                   object --+
                            |
                 named._Named --+
                                |
                 named._NamedBase --+
                                    |
                latlonBase.LatLonBase --+
                                        |
    ellipsoidalBase.LatLonEllipsoidalBase --+
                                            |
                                           LatLonEllipsoidalBaseDI

Known Subclasses:
  - ellipsoidalExact.LatLon
  - , ellipsoidalGeodSolve.LatLon
  - , ellipsoidalKarney.LatLon
  - , ellipsoidalVincenty.LatLon

(INTERNAL) Base class for `ellipsoidal*.LatLon` classes with overloaded `Direct` and `Inverse` methods.

Instance Methods
bearingTo2(self, other, wrap=False) Compute the initial and final bearing (forward and reverse azimuth) from this to an other point, using this `Inverse` method. |
destination(self, distance, bearing, height=None) Compute the destination point after having travelled for the given distance from this point along a geodesic given by an initial bearing, using this `Direct` method. |
destination2(self, distance, bearing, height=None) Compute the destination point and the final bearing (reverse azimuth) after having travelled for the given distance from this point along a geodesic given by an initial bearing, using this `Direct` method. |
distanceTo(self, other, wrap=False, **unused) Compute the distance between this and an other point along a geodesic, using this `Inverse` method. |
distanceTo3(self, other, wrap=False) Compute the distance, the initial and final bearing along a geodesic between this and an other point, using this `Inverse` method. |
finalBearingOn(self, distance, bearing) Compute the final bearing (reverse azimuth) after having travelled for the given distance along a geodesic given by an initial bearing from this point, using this `Direct` method. |
finalBearingTo(self, other, wrap=False) Compute the final bearing (reverse azimuth) after having travelled along a geodesic from this point to an other point, using this `Inverse` method. |
initialBearingTo(self, other, wrap=False) Compute the initial bearing (forward azimuth) to travel along a geodesic from this point to an other point, using this `Inverse` method. |
intermediateTo(self, other, fraction, height=None, wrap=False) Return the point at given fraction along the geodesic between this and an other point, using this `Direct` and `Inverse` methods. |
intersecant2(self, circle, point, other, exact=False, height=None, wrap=False, tol=1.4901161193847656e-08) Compute the intersections of a circle and a geodesic (line) given as two points or as a point and bearing. |
nearestOn8(self, points, closed=False, height=None, wrap=False, equidistant=None, tol=0.001) Iteratively locate the point on a path or polygon closest to this point. |
plumbTo(self, point, other, exact=False, height=None, wrap=False, tol=1.4901161193847656e-08) Compute the perpendicular intersection of a geodesic (line) with a geodesic from this point. |
Inherited from `ellipsoidalBase.LatLonEllipsoidalBase`: `__init__`, `antipode`, `convertDatum`, `convertRefFrame`, `distanceTo2`, `elevation2`, `ellipsoid`, `ellipsoids`, `geoidHeight2`, `intersection3`, `intersections2`, `isenclosedBy`, `midpointTo`, `nearestOn`, `parse`, `to3xyz`, `toCss`, `toDatum`, `toEtm`, `toLcc`, `toMgrs`, `toOsgr`, `toRefFrame`, `toUps`, `toUtm`, `toUtmUps`, `triangulate`, `trilaterate5` Inherited from `latlonBase.LatLonBase`: `PointsIter`, `__eq__`, `__ne__`, `__str__`, `bounds`, `boundsOf`, `chordTo`, `circin6`, `circum3`, `circum4_`, `compassAngle`, `compassAngleTo`, `cosineAndoyerLambertTo`, `cosineForsytheAndoyerLambertTo`, `cosineLawTo`, `destinationXyz`, `equals`, `equals3`, `equirectangularTo`, `euclideanTo`, `flatLocalTo`, `flatPolarTo`, `hartzell`, `haversineTo`, `height4`, `heightStr`, `hubenyTo`, `isantipode`, `isantipodeTo`, `isequalTo`, `isequalTo3`, `latlon2`, `latlon2round`, `latlon_`, `nearestOn6`, `nearestTo`, `normal`, `philam2`, `points`, `points2`, `radii11`, `rhumbAzimuthTo`, `rhumbDestination`, `rhumbDistanceTo`, `rhumbIntersecant2`, `rhumbLine`, `rhumbMidpointTo`, `thomasTo`, `to2ab`, `to3llh`, `toCartesian`, `toEcef`, `toLocal`, `toLtp`, `toNormal`, `toNvector`, `toStr`, `toVector`, `toVector3d`, `toWm`, `vincentysTo` Inherited from `named._NamedBase`: `__repr__`, `others`, `toRepr` Inherited from `named._Named`: `__imatmul__`, `__matmul__`, `__rmatmul__`, `attrs`, `classof`, `copy`, `dup`, `methodname`, `rename`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
| geodesic N/A, invalid (`None` always).
Inherited from `ellipsoidalBase.LatLonEllipsoidalBase`: `Equidistant`, `convergence`, `datum`, `ellipsoidalLatLon`, `epoch`, `gamma`, `iteration`, `reframe`, `scale` Inherited from `latlonBase.LatLonBase`: `Ecef`, `clipid`, `height`, `isEllipsoidal`, `isSpherical`, `isnormal`, `lam`, `lat`, `latlon`, `latlonheight`, `lon`, `phi`, `philam`, `philamheight`, `sphericalLatLon`, `xyz`, `xyzh` Inherited from `named._Named`: `classname`, `classnaming`, `name`, `named`, `named2`, `named3`, `named4`, `sizeof` Inherited from `object`: `__class__`

Method Details

### bearingTo2 (self, other, wrap=False) |
Compute the initial and final bearing (forward and reverse azimuth) from this to an other point, using this `Inverse` method. See methods initialBearingTo and finalBearingTo for more details. Arguments: `other` - The other point (`LatLon`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: A Bearing2Tuple`(initial, final)`. Raises: `TypeError` - The `other` point is not `LatLon`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible.

### destination (self, distance, bearing, height=None) |
Compute the destination point after having travelled for the given distance from this point along a geodesic given by an initial bearing, using this `Direct` method. See method destination2 for more details. Arguments: `distance` - Distance (`meter`). `bearing` - Initial bearing in (compass `degrees360`). `height` - Optional height, overriding the default height (`meter`, same units as `distance`). Returns: The destination point (`LatLon`).

### destination2 (self, distance, bearing, height=None) |
Compute the destination point and the final bearing (reverse azimuth) after having travelled for the given distance from this point along a geodesic given by an initial bearing, using this `Direct` method. The distance must be in the same units as this point's datum axes, conventionally `meter`. The distance is measured on the surface of the ellipsoid, ignoring this point's height. The initial and final bearing (forward and reverse azimuth) are in compass `degrees360`. The destination point's height and datum are set to this point's height and datum, unless the former is overridden. Arguments: `distance` - Distance (`meter`). `bearing` - Initial bearing (compass `degrees360`). `height` - Optional height, overriding the default height (`meter`, same units as `distance`). Returns: A Destination2Tuple`(destination, final)`.

### distanceTo (self, other, wrap=False, **unused) |
Compute the distance between this and an other point along a geodesic, using this `Inverse` method. See method distanceTo3 for more details. Arguments: `other` - The other point (`LatLon`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: Distance (`meter`). Raises: `TypeError` - The `other` point is not `LatLon`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible.

### distanceTo3 (self, other, wrap=False) |
Compute the distance, the initial and final bearing along a geodesic between this and an other point, using this `Inverse` method. The distance is in the same units as this point's datum axes, conventionally meter. The distance is measured on the surface of the ellipsoid, ignoring this point's height. The initial and final bearing (forward and reverse azimuth) are in compass `degrees360` from North. Arguments: `other` - Destination point (`LatLon`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: A Distance3Tuple`(distance, initial, final)`. Raises: `TypeError` - The `other` point is not `LatLon`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible.

### finalBearingOn (self, distance, bearing) |
Compute the final bearing (reverse azimuth) after having travelled for the given distance along a geodesic given by an initial bearing from this point, using this `Direct` method. See method destination2 for more details. Arguments: `distance` - Distance (`meter`). `bearing` - Initial bearing (compass `degrees360`). Returns: Final bearing (compass `degrees360`).

### finalBearingTo (self, other, wrap=False) |
Compute the final bearing (reverse azimuth) after having travelled along a geodesic from this point to an other point, using this `Inverse` method. See method distanceTo3 for more details. Arguments: `other` - The other point (`LatLon`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: Final bearing (compass `degrees360`). Raises: `TypeError` - The `other` point is not `LatLon`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible.

### initialBearingTo (self, other, wrap=False) |
Compute the initial bearing (forward azimuth) to travel along a geodesic from this point to an other point, using this `Inverse` method. See method distanceTo3 for more details. Arguments: `other` - The other point (`LatLon`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: Initial bearing (compass `degrees360`). Raises: `TypeError` - The `other` point is not `LatLon`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible.

### intermediateTo (self, other, fraction, height=None, wrap=False) |
Return the point at given fraction along the geodesic between this and an other point, using this `Direct` and `Inverse` methods. Arguments: `other` - The other point (`LatLon`). `fraction` - Fraction between both points (`scalar`, 0.0 at this and 1.0 at the other point. `height` - Optional height, overriding the fractional height (`meter`). `wrap` - If `True`, wrap or normalize and unroll the `other` point (`bool`). Returns: Intermediate point (`LatLon`). Raises: `TypeError` - The `other` point is not `LatLon`. `UnitError` - Invalid `fraction` or `height`. `ValueError` - If this and the `other` point's Datum ellipsoids are not compatible. Overrides: ellipsoidalBase.LatLonEllipsoidalBase.intermediateTo See Also: Methods distanceTo3, destination, `midpointTo` and `rhumbMidpointTo`.

### intersecant2 (self, circle, point, other, exact=False, height=None, wrap=False, tol=1.4901161193847656e-08) |
Compute the intersections of a circle and a geodesic (line) given as two points or as a point and bearing. Arguments: `circle` - Radius of the circle centered at this location (`meter`, conventionally) or a point on the circle (this `LatLon`). `point` - A location on the geodesic (this `LatLon`). `other` - An other point on the geodesic (this `LatLon`) or the (forward) bearing at the `point` (compass `degrees`). `exact` - Exact `geodesic...` to use (`bool` or `Geodesic...`), see method Ellipsoid.geodesic_. `height` - Optional height for the intersection points (`meter`, conventionally) or `None` for interpolated heights. `wrap` - If `True`, wrap or normalize and unroll the `point`, `circle` and/or `other` (`bool`). `tol` - Convergence tolerance (`scalar`). Returns: 2-Tuple of the intersection points (representing a geodesic chord), each an instance of this `LatLon`. Both points are the same instance if the geodesic (line) is tangential to the circle. Raises: `IntersectionError` - The circle and geodesic do not intersect. `TypeError` - If `point` is not this `LatLon` or `circle` or `other` invalid. `UnitError` - Invalid `circle`, `other`, `exact` or `height`. Overrides: latlonBase.LatLonBase.intersecant2 See Also: Method rhumbIntersecant2.

### nearestOn8 (self, points, closed=False, height=None, wrap=False, equidistant=None, tol=0.001) |
Iteratively locate the point on a path or polygon closest to this point. Arguments: `points` - The path or polygon points (`LatLon`[]). `closed` - Optionally, close the polygon (`bool`). `height` - Optional height, overriding the height of this and all other points (`meter`, conventionally). If `height` is `None`, the height of each point is taken into account for distances. `wrap` - If `True`, wrap or normalize and unroll the `points` (`bool`). Returns: A NearestOn8Tuple`(closest, distance, fi, j, start, end, initial, final)` with `distance` in `meter`, conventionally and with the `closest`, the `start` the `end` point each an instance of this `LatLon`. Raises: `PointsError` - Insufficient number of `points`. `TypeError` - Some `points` or `equidistant` invalid. `ValueError` - Some `points`' datum or ellipsoid incompatible or no convergence for the given `tol`. See Also: Function pygeodesy.nearestOn6 and method `nearestOn6`.

### plumbTo (self, point, other, exact=False, height=None, wrap=False, tol=1.4901161193847656e-08) |
Compute the perpendicular intersection of a geodesic (line) with a geodesic from this point. Arguments: `point` - A location (`LatLon`) on the geodesic (line). `other` - An other point (`LatLon`) on the geodesic (line) or the (forward) bearing at the `point` (compass `degrees`). `exact` - Exact `geodesic...` to use (`bool` or `Geodesic...`), see method Ellipsoid.geodesic_. `height` - Optional height for the intersection point (`meter`, conventionally) or `None` for an interpolated height. `wrap` - If `True`, wrap or normalize and unroll the `point` and/or `other` (`bool`). `tol` - Convergence tolerance (`scalar`). Returns: The intersection point, an instance of this `LatLon`. Raises: `TypeError` - If `point` or `other` not this `LatLon`. `UnitError` - Invalid `other`, `exact` or `height`.

Property Details

### geodesic N/A, invalid (`None` always). Get method: geodesic(self) - N/A, invalid (`None` always). Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst) - Zap the cached/memoized `property` value.