Package pygeodesy :: Module errors |
[frames] | no frames]

# Module errors

Errors, exceptions and exception chaining.

Error, exception classes and functions to format PyGeodesy errors, including the setting of exception chaining in Python 3+.

By default, exception chaining is turned off. To enable exception chaining, use command line option `python -X dev` OR set env var `PYTHONDEVMODE` to `1` or any non-empyty string OR set env var `PYGEODESY_EXCEPTION_CHAINING=std` or any other non-empty string.

Version: 22.03.02

Classes
| CrossError Error raised for zero or near-zero vectorial cross products, occurring for coincident or colinear points, paths or bearings.
| IntersectionError Error raised for path or circle intersection issues.
| LenError Error raised for mis-matching `len` values.
| LimitError Error raised for lat- or longitudinal deltas exceeding the `limit` in functions pygeodesy.equirectangular and pygeodesy.equirectangular_ and several `nearestOn*` and `simplify*` functions or methods.
| NumPyError Error raised for `NumPy` errors.
| PointsError Error for an insufficient number of points.
| RangeError Error raised for lat- or longitude values outside the `clip`, `clipLat`, `clipLon` or `limit` range in function pygeodesy.clipDegrees, pygeodesy.clipRadians, pygeodesy.parse3llh, pygeodesy.parseDMS, pygeodesy.parseDMS2 or pygeodesy.parseRad.
| TriangleError Error raised for triangle, inter- or resection issues.
| SciPyError Error raised for `SciPy` errors.
| SciPyWarning Error thrown for `SciPy` warnings.
| TRFError Terrestrial Reference Frame (TRF), Epoch, RefFrame or RefFrame conversion issue.
| UnitError Default exception for units issues.
| VectorError Vector3d, `Cartesian*` or `*Nvector` issues.

Functions
crosserrors(raiser=None) Report or ignore vectorial cross product errors. |
exception_chaining(error=None) Get the previous exception's or exception chaining setting. |
limiterrors(raiser=None) Get/set the throwing of LimitErrors. |
rangerrors(raiser=None) Get/set the throwing of RangeErrors. |

Variables
| __all__ = `_ALL_LAZY.errors`
| _ = `{}.__or__`

Function Details

### crosserrors (raiser=None) |
Report or ignore vectorial cross product errors. Arguments: `raiser` - Use `True` to throw or `False` to ignore CrossError exceptions. Use `None` to leave the setting unchanged. Returns: Previous setting (`bool`). See Also: Property `Vector3d[Base].crosserrors`.

### exception_chaining (error=None) |
Get the previous exception's or exception chaining setting. Arguments: `error` - An error instance (`Exception`) or `None`. Returns: If `error is None`, return `True` if exception chaining is enabled for PyGeodesy errors, `False` if turned off and `None` if not available. If `error` is not `None`, return the previous, chained error or `None` otherwise. Note: Set env var `PYGEODESY_EXCEPTION_CHAINING` to any non-empty value prior to `import pygeodesy` to enable exception chaining for `pygeodesy` errors.

### limiterrors (raiser=None) |
Get/set the throwing of LimitErrors. Arguments: `raiser` - Choose `True` to raise or `False` to ignore LimitError exceptions. Use `None` to leave the setting unchanged. Returns: Previous setting (`bool`).

### rangerrors (raiser=None) |
Get/set the throwing of RangeErrors. Arguments: `raiser` - Choose `True` to raise or `False` to ignore RangeError exceptions. Use `None` to leave the setting unchanged. Returns: Previous setting (`bool`).