Package pygeodesy :: Package deprecated :: Module datum |
[frames] | no frames]

# Module datum

DEPRECATED, use module datums or ellipsoids instead.

Version: 22.09.12

Classes
| Ellipsoid Ellipsoid with equatorial and polar radii, flattening, inverse flattening and other, often used, cached attributes, supporting oblate and prolate ellipsoidal and spherical earth models.
| Curvature2Tuple 2-Tuple `(meridional, prime_vertical)` of radii of curvature, both in `meter`, conventionally.
| Datum Ellipsoid and transform parameters for an earth model.
| Transform Helmert transformation.

Variables
| R_M = `6371008.771415`
| R_MA = `6378137.0`
| R_MB = `6356752.3`
| R_KM = `6371.0087714149995`
| R_NM = `3440.06953100162`
| R_SM = `3958.7613160486508`
| R_FM = `6371000.0`
| R_VM = `6366707.0194937`
| Ellipsoids = `Ellipsoids.Sphere: Ellipsoid(name='Sphere', a=637`...``
| Datums = `Datums.OSGB36: Datum(name='OSGB36', ellipsoid=Ellipso`...``
| Transforms = `Transforms.OSGB36: Transform(name='OSGB36', tx=-4`...``

Variables Details

  ### Ellipsoids Value:
      Ellipsoids.Sphere: Ellipsoid(name='Sphere', a=6371008.771415, b=637100
      8.771415, f_=0, f=0, f2=0, n=0, e=0, e2=0, e22=0, e32=0, A=6371008.771
      415, L=10007557.17611675, R1=6371008.771415, R2=6371008.771415, R3=637
      1008.771415, Rbiaxial=6371008.771415, Rtriaxial=6371008.771415),
      Ellipsoids.WGS84: Ellipsoid(name='WGS84', a=6378137, b=6356752.3142451
      8, f_=298.25722356, f=0.00335281, f2=0.00336409, n=0.00167922, e=0.081
      81919, e2=0.00669438, e22=0.0067395, e32=0.00335843, A=6367449.1458234
      1, L=10001965.72931272, R1=6371008.77141506, R2=6371007.18091847, R3=6
      ...

  ### Datums Value:
      Datums.OSGB36: Datum(name='OSGB36', ellipsoid=Ellipsoids.Airy1830, tra
      nsform=Transforms.OSGB36),
      Datums.WGS84: Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transfor
      m=Transforms.WGS84),
      Datums.Sphere: Datum(name='Sphere', ellipsoid=Ellipsoids.Sphere, trans
      form=Transforms.WGS84)

  ### Transforms Value:
      Transforms.OSGB36: Transform(name='OSGB36', tx=-446.448, ty=125.157, t
      z=-542.06, rx=-0, ry=-0, rz=-0, s=20.4894, s1=1.00002, sx=-0.1502, sy=
      -0.247, sz=-0.8421),
      Transforms.WGS84: Transform(name='WGS84', tx=0, ty=0, tz=0, rx=0, ry=0
      , rz=0, s=0, s1=1, sx=0, sy=0, sz=0)